|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Macros | Functions
WDT Driver
MPLABX MCC Melody Code Generator

Watchdog Timer Driver using dsPIC MCUs. More...

Collaboration diagram for WDT Driver:

## Macros
#define | WATCHDOG_CLR_KEY 0x5743
| This macro holds the key value to clear Watchdog Timer (WDT)

## Functions
static void | WATCHDOG_TimerSoftwareEnable (void)
| This inline function is used to enable the Watchdog Timer (WDT) using the software bit.
static void | WATCHDOG_TimerSoftwareDisable (void)
| This inline function is used to disable the Watchdog Timer (WDT) using the software bit.
static void | WATCHDOG_TimerClear (void)
| This inline function is used to clear the Watchdog Timer (WDT)

## Detailed Description

## Macro Definition Documentation

## ◆ WATCHDOG_CLR_KEY

#define WATCHDOG_CLR_KEY 0x5743

Definition at line 48 of file watchdog.h.

## Function Documentation

## ◆ WATCHDOG_TimerClear()

static void WATCHDOG_TimerClear | ( | void |  | ) |
| inlinestatic

Parameters

  none |

Returns
  none

Definition at line 78 of file watchdog.h.

## ◆ WATCHDOG_TimerSoftwareDisable()

static void WATCHDOG_TimerSoftwareDisable | ( | void |  | ) |
| inlinestatic

Parameters

  none |

Returns
  none

Definition at line 67 of file watchdog.h.

## ◆ WATCHDOG_TimerSoftwareEnable()

static void WATCHDOG_TimerSoftwareEnable | ( | void |  | ) |
| inlinestatic

Parameters

  none |

Returns
  none

Definition at line 56 of file watchdog.h.