<config configName="default" projectName="dab-pwm-configuration" configVersion="1.1" device="dsPIC33CK256MP506" deviceLibraryClass="com.microchip.mcc.melody.Library" coreVersion="5.7.1">
   <usedPackages class="java.util.ArrayList">
      <package packageName="@mchp-mcc/adc-multicore-driver" version="2.1.4" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/can-fd-driver" version="1.2.2" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/clc-16bit-driver" version="1.0.6-dev.1" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/clock-16bit-driver" version="1.2.1" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/cmp-dac-driver" version="1.0.5" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/crc-16bit-driver" version="1.0.3" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/dmt-16bit-driver" version="1.0.6" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/dspic33-configuration-bits" version="1.2.2" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/icd-16bit-driver" version="1.0.3" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/main-16bit-manager" version="1.1.2" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic-16bit" version="5.11.4" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-adc-multicore" version="2.4.3" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-can-fd-upb" version="1.7.0" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-cla-clc-upb" version="1.3.0" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-clock-sib" version="1.4.2" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-cmp-dac" version="1.4.2" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-crc-upb" version="1.3.0" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-dmt-upb" version="1.1.1" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-interrupt" version="1.3.1" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-mccp-upb" version="1.6.4" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-pin-manager" version="1.3.0" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-pwm-pc-upb" version="2.4.2" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-reset" version="1.1.0" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-tmr-class-upb" version="1.5.3" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-uart-protocol-upb" version="1.5.0" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pic24-dspic33-wdt-upb-v1" version="1.2.1" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pin-content-processor" version="3.8.0" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pwm-driver" version="1.0.5" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/pwm-hs-driver" version="2.2.1" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/timer" version="1.2.1" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/uart-driver" version="1.10.1" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
      <package packageName="@mchp-mcc/wdt-16bit-driver" version="1.0.8" contentType="MELODY">
         <modules class="java.util.ArrayList"/>
      </package>
   </usedPackages>
   <usedClasses class="java.util.TreeMap">
      <entry>
         <string>ADC1</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>Application Builder</string>
         <string>class com.microchip.mcc.melody.module.FrameworkModule</string>
      </entry>
      <entry>
         <string>CAN1</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>CLC1</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>CMP1</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>CMP2</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>CMP3</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>CRC</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>Configuration Bits</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>DMT</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>ICD</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>INTERNAL OSCILLATOR</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>INTERRUPT CORE</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>MAIN MANAGER</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>PWM</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>Pin Manager</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>RESET</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>SCCP1</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>SCCP3</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>TMR1</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>UART1</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>WATCHDOG</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>meta</string>
         <string>class com.microchip.mcc.melody.hw.module.HardwareModule</string>
      </entry>
      <entry>
         <string>module0</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module1</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module102</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module104</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module107</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module109</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module111</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module12</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module128</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module130</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module2</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module20</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module23</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module25</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module3</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module31</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module33</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module34</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module35</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module36</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module39</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module4</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module43</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module44</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module46</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module5</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module50</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module6</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module66</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module7</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module70</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module71</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module79</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module84</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module90</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module92</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
      <entry>
         <string>module94</string>
         <string>class com.microchip.mcc.melody.script.module.ScriptModule</string>
      </entry>
   </usedClasses>
   <usedLibraries class="java.util.ArrayList">
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.melody.Library" version="2.7.1"/>
   </usedLibraries>
   <tokenMap class="java.util.TreeMap">
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Application Builder" name="graph-location-data"/>
         <value>{&quot;mccDevice&quot;:{&quot;loc&quot;:&quot;0 0&quot;,&quot;pos&quot;:&quot;0 0&quot;},&quot;systemGroup&quot;:{&quot;loc&quot;:&quot;0 -107&quot;,&quot;pos&quot;:&quot;0 -107&quot;},&quot;module43&quot;:{&quot;loc&quot;:&quot;196 0&quot;,&quot;pos&quot;:&quot;196 0&quot;},&quot;module20&quot;:{&quot;loc&quot;:&quot;196 -770&quot;,&quot;pos&quot;:&quot;196 -770&quot;},&quot;module25&quot;:{&quot;loc&quot;:&quot;196 -616&quot;,&quot;pos&quot;:&quot;196 -616&quot;},&quot;module46&quot;:{&quot;loc&quot;:&quot;393 -77&quot;,&quot;pos&quot;:&quot;393 -77&quot;},&quot;module23&quot;:{&quot;loc&quot;:&quot;196 -693&quot;,&quot;pos&quot;:&quot;196 -693&quot;},&quot;module44&quot;:{&quot;loc&quot;:&quot;196 -539&quot;,&quot;pos&quot;:&quot;196 -539&quot;},&quot;module111&quot;:{&quot;loc&quot;:&quot;393 -693&quot;,&quot;pos&quot;:&quot;393 -693&quot;},&quot;module130&quot;:{&quot;loc&quot;:&quot;393 -154&quot;,&quot;pos&quot;:&quot;393 -154&quot;},&quot;module7&quot;:{&quot;loc&quot;:&quot;196 -77&quot;,&quot;pos&quot;:&quot;196 -77&quot;},&quot;module39&quot;:{&quot;loc&quot;:&quot;196 -847&quot;,&quot;pos&quot;:&quot;196 -847&quot;},&quot;module107&quot;:{&quot;loc&quot;:&quot;393 -231&quot;,&quot;pos&quot;:&quot;393 -231&quot;},&quot;module109&quot;:{&quot;loc&quot;:&quot;393 -462&quot;,&quot;pos&quot;:&quot;393 -462&quot;},&quot;module36&quot;:{&quot;loc&quot;:&quot;196 -231&quot;,&quot;pos&quot;:&quot;196 -231&quot;},&quot;module104&quot;:{&quot;loc&quot;:&quot;393 -385&quot;,&quot;pos&quot;:&quot;393 -385&quot;},&quot;module35&quot;:{&quot;loc&quot;:&quot;196 -308&quot;,&quot;pos&quot;:&quot;196 -308&quot;},&quot;module34&quot;:{&quot;loc&quot;:&quot;196 -385&quot;,&quot;pos&quot;:&quot;196 -385&quot;},&quot;module12&quot;:{&quot;loc&quot;:&quot;196 -154&quot;,&quot;pos&quot;:&quot;196 -154&quot;},&quot;module33&quot;:{&quot;loc&quot;:&quot;196 -462&quot;,&quot;pos&quot;:&quot;196 -462&quot;},&quot;module128&quot;:{&quot;loc&quot;:&quot;393 -308&quot;,&quot;pos&quot;:&quot;393 -308&quot;},&quot;module90&quot;:{&quot;loc&quot;:&quot;393 -539&quot;,&quot;pos&quot;:&quot;393 -539&quot;},&quot;module102&quot;:{&quot;loc&quot;:&quot;393 -616&quot;,&quot;pos&quot;:&quot;393 -616&quot;},&quot;module94&quot;:{&quot;loc&quot;:&quot;393 0&quot;,&quot;pos&quot;:&quot;393 0&quot;},&quot;module70&quot;:{&quot;loc&quot;:&quot;393 -770&quot;,&quot;pos&quot;:&quot;393 -770&quot;},&quot;module92&quot;:{&quot;loc&quot;:&quot;393 -847&quot;,&quot;pos&quot;:&quot;393 -847&quot;}}</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Application Builder" name="state"/>
         <value>{&quot;userAddedModules&quot;:[&quot;module84&quot;,&quot;module46&quot;,&quot;module66&quot;,&quot;module111&quot;,&quot;module130&quot;,&quot;module5&quot;,&quot;module4&quot;,&quot;module6&quot;,&quot;module1&quot;,&quot;module0&quot;,&quot;module3&quot;,&quot;module2&quot;,&quot;module107&quot;,&quot;module31&quot;,&quot;module109&quot;,&quot;module79&quot;,&quot;module104&quot;,&quot;module128&quot;,&quot;module90&quot;,&quot;module102&quot;,&quot;module50&quot;,&quot;module94&quot;,&quot;module71&quot;,&quot;module70&quot;,&quot;module92&quot;],&quot;version&quot;:&quot;CURRENT&quot;,&quot;modules&quot;:{&quot;module43&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-adc-multicore&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;adc_pc_ctrl_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;adc_pc_ctrl_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;ADC1&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;hardware&quot;:{&quot;clkselAdcon3h&quot;:&quot;FOSC/2&quot;}}}},&quot;module20&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-tmr-class-upb&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;tmr_classa_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;tmr_classa_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;TMR1&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module84&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/dmt-16bit-driver&quot;,&quot;imports&quot;:{&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;dmt_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;dmt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module50&quot;,&quot;exportId&quot;:&quot;dmt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module25&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-mccp-upb&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;ccp_mccp_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;ccp_mccp_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;SCCP3&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;hide&quot;:{&quot;ocaenPinData&quot;:{&quot;RC8&quot;:{&quot;cname&quot;:&quot;IO_RC8&quot;}}}}}},&quot;module46&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/can-fd-driver&quot;,&quot;imports&quot;:{&quot;can_fd_basic&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;can-fd-interface&quot;,&quot;version&quot;:&quot;^1.1.1&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module7&quot;,&quot;exportId&quot;:&quot;can_basic&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;clockSettings&quot;:{&quot;requestedSpeed&quot;:&quot;40.00 MHz&quot;},&quot;nominalBitRateSetting&quot;:{&quot;nominalBitRate&quot;:&quot;1 Mbps&quot;},&quot;dataBitRateSetting&quot;:{&quot;enableDataBitRateSetting&quot;:true,&quot;dataBitRate&quot;:&quot;4 Mbps&quot;},&quot;fifoSetting&quot;:{&quot;fifoTable&quot;:[{&quot;rowId&quot;:0.0,&quot;uid&quot;:&quot;dynamicRow_0&quot;,&quot;enable&quot;:true,&quot;depth&quot;:&quot;3&quot;,&quot;payload&quot;:&quot;64&quot;},{&quot;rowId&quot;:1.0,&quot;uid&quot;:&quot;dynamicRow_1&quot;,&quot;operation&quot;:&quot;RX&quot;,&quot;payload&quot;:&quot;64&quot;,&quot;enable&quot;:true},{&quot;rowId&quot;:2.0,&quot;uid&quot;:&quot;dynamicRow_2&quot;,&quot;operation&quot;:&quot;RX&quot;,&quot;payload&quot;:&quot;64&quot;,&quot;enable&quot;:true}]},&quot;Filter0&quot;:{&quot;enableFilter0&quot;:true,&quot;msgIdFilter0&quot;:&quot;0x402&quot;},&quot;Filter1&quot;:{&quot;enableFilter1&quot;:true,&quot;msgIdFilter1&quot;:&quot;0x403&quot;,&quot;receiveFifoFilter1&quot;:&quot;FIFO2&quot;}}}},&quot;module23&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-mccp-upb&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;ccp_mccp_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;ccp_mccp_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;SCCP1&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module66&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-reset&quot;,&quot;imports&quot;:{&quot;rst_sib_v2&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;rst_sib_v2&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;RESET&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module44&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-pwm-pc-upb&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;pwm_pc_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pwm_pc_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;PWM&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;hide&quot;:{&quot;pwm1-hPinData&quot;:{&quot;RB14&quot;:{&quot;cname&quot;:&quot;IO_RB14&quot;}},&quot;pwm1-lPinData&quot;:{&quot;RB15&quot;:{&quot;cname&quot;:&quot;IO_RB15&quot;}},&quot;pwm2-hPinData&quot;:{&quot;RB12&quot;:{&quot;cname&quot;:&quot;IO_RB12&quot;}},&quot;pwm2-lPinData&quot;:{&quot;RB13&quot;:{&quot;cname&quot;:&quot;IO_RB13&quot;}},&quot;pwm3-hPinData&quot;:{&quot;RB10&quot;:{&quot;cname&quot;:&quot;IO_RB10&quot;}},&quot;pwm3-lPinData&quot;:{&quot;RB11&quot;:{&quot;cname&quot;:&quot;IO_RB11&quot;}},&quot;pwm4-hPinData&quot;:{&quot;RD1&quot;:{&quot;cname&quot;:&quot;IO_RD1&quot;}},&quot;pwm4-lPinData&quot;:{&quot;RD0&quot;:{&quot;cname&quot;:&quot;IO_RD0&quot;}},&quot;pwm4hPinData&quot;:{},&quot;pwm4lPinData&quot;:{},&quot;pwm6-hPinData&quot;:{&quot;RC14&quot;:{&quot;cname&quot;:&quot;IO_RC14&quot;}},&quot;pwm6-lPinData&quot;:{&quot;RC15&quot;:{&quot;cname&quot;:&quot;IO_RC15&quot;}}},&quot;software&quot;:{&quot;clockSource&quot;:&quot;AFVCO/2&quot;}}}},&quot;module111&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/timer&quot;,&quot;imports&quot;:{&quot;timer_periodic&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;timer-periodic&quot;,&quot;version&quot;:&quot;^2.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module23&quot;,&quot;exportId&quot;:&quot;basic_ccp&quot;,&quot;label&quot;:&quot;SCCP1&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[&quot;timer_periodic&quot;]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;customName&quot;:&quot;CTRLLOOP_EXE&quot;,&quot;requestedTimerPeriod&quot;:{&quot;value&quot;:10.0,&quot;unit&quot;:&quot;us&quot;}}}}},&quot;module130&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/clc-16bit-driver&quot;,&quot;imports&quot;:{&quot;clc_basic&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clc-basic&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module12&quot;,&quot;exportId&quot;:&quot;clc_basic&quot;,&quot;label&quot;:&quot;CLC1&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[&quot;clc_basic&quot;]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;clcMode&quot;:&quot;OR-XOR&quot;,&quot;dataInput4&quot;:&quot;CMP3 output&quot;,&quot;gate4Input4State&quot;:&quot;Non-Inverted&quot;,&quot;dataInput2&quot;:&quot;CMP1 output&quot;,&quot;gate2Input2State&quot;:&quot;Non-Inverted&quot;,&quot;gate1Input2State&quot;:&quot;Non-Inverted&quot;,&quot;gate3Input4State&quot;:&quot;Non-Inverted&quot;}}}},&quot;module5&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-clock-sib&quot;,&quot;imports&quot;:{&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;clk_sib_v12&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clk_sib_v12&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;INTERNAL OSCILLATOR&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;config_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;config-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module1&quot;,&quot;exportId&quot;:&quot;config_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;clockOutputPinConfig&quot;:&quot;OSC2 is general purpose digital i/o pin&quot;}}}},&quot;module4&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pin-content-processor&quot;,&quot;imports&quot;:{&quot;device-meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;pin-architecture&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-architecture&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module3&quot;,&quot;exportId&quot;:&quot;pin-architecture&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;saved&quot;:{&quot;rows&quot;:{&quot;module39&quot;:{&quot;UART1$U1TX$output&quot;:{&quot;pins&quot;:{&quot;RD3&quot;:{&quot;state&quot;:&quot;L&quot;}}}},&quot;pcp&quot;:{&quot;GPIO$GPIO$input&quot;:{&quot;pins&quot;:{&quot;RD2&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RD7&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RC10&quot;:{&quot;state&quot;:&quot;MUL&quot;},&quot;RC11&quot;:{&quot;state&quot;:&quot;MUL&quot;},&quot;RD12&quot;:{&quot;state&quot;:&quot;MUL&quot;},&quot;RD15&quot;:{&quot;state&quot;:&quot;MUL&quot;},&quot;RD8&quot;:{&quot;state&quot;:&quot;MUL&quot;},&quot;RD9&quot;:{&quot;state&quot;:&quot;MUL&quot;},&quot;RC4&quot;:{&quot;state&quot;:&quot;UL&quot;},&quot;RC15&quot;:{&quot;state&quot;:&quot;UL&quot;},&quot;RB9&quot;:{&quot;state&quot;:&quot;UL&quot;},&quot;RC14&quot;:{&quot;state&quot;:&quot;MUL&quot;}}},&quot;GPIO$GPIO$output&quot;:{&quot;pins&quot;:{&quot;RD2&quot;:{&quot;state&quot;:&quot;MUL&quot;},&quot;RD7&quot;:{&quot;state&quot;:&quot;MUL&quot;},&quot;RC10&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RC11&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RD12&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RD15&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RD8&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RD9&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RC4&quot;:{&quot;state&quot;:&quot;UL&quot;},&quot;RC15&quot;:{&quot;state&quot;:&quot;UL&quot;},&quot;RB9&quot;:{&quot;state&quot;:&quot;UL&quot;},&quot;RC14&quot;:{&quot;state&quot;:&quot;L&quot;}}}},&quot;module7&quot;:{&quot;CAN1$CAN1TX$output&quot;:{&quot;pins&quot;:{&quot;RD5&quot;:{&quot;state&quot;:&quot;L&quot;}}}},&quot;module25&quot;:{&quot;SCCP3$OCM3$output&quot;:{&quot;pins&quot;:{&quot;RC8&quot;:{&quot;state&quot;:&quot;L&quot;},&quot;RB14&quot;:{&quot;state&quot;:&quot;UL&quot;}}}}},&quot;userEditedData&quot;:{&quot;inputPPSState&quot;:{&quot;module39&quot;:{&quot;UART1&quot;:{&quot;U1RX&quot;:&quot;RD4&quot;}},&quot;module7&quot;:{&quot;CAN1&quot;:{&quot;CAN1RX&quot;:&quot;RD6&quot;}},&quot;module12&quot;:{&quot;CLC1&quot;:{&quot;CLCINC&quot;:&quot;&quot;}}},&quot;cname&quot;:{&quot;eview&quot;:{&quot;RD7&quot;:&quot;LED_GREEN&quot;,&quot;RC10&quot;:&quot;GPIO_1&quot;,&quot;RC11&quot;:&quot;GPIO_2&quot;,&quot;RD12&quot;:&quot;TP_PIM&quot;,&quot;RD15&quot;:&quot;LED_DP_PIM&quot;,&quot;RD8&quot;:&quot;LED_RED&quot;,&quot;RD9&quot;:&quot;FAULT&quot;,&quot;RC14&quot;:&quot;DPD_TP31&quot;}},&quot;high&quot;:{&quot;eview&quot;:{&quot;RD9&quot;:true}},&quot;odc&quot;:{&quot;eview&quot;:{&quot;RD9&quot;:true}}}}}},&quot;module7&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-can-fd-upb&quot;,&quot;imports&quot;:{&quot;canfd_clock&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;canfd-clock-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module6&quot;,&quot;exportId&quot;:&quot;canfd_clock&quot;}},&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}},&quot;can_fd_upb_v2&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;can_fd_upb_v2&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;CAN1&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module6&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/clock-16bit-driver&quot;,&quot;imports&quot;:{&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;clock_16bit_config_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-config-interface&quot;,&quot;version&quot;:&quot;^1.1.5&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_config_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;systemClock&quot;:{&quot;mainClockSource&quot;:&quot;FRC Oscillator with PLL&quot;,&quot;setMaximumSystemFrequency&quot;:true,&quot;fvcoDivider&quot;:&quot;2&quot;},&quot;auxClock&quot;:{&quot;auxClockSource&quot;:&quot;FRC Oscillator with PLL&quot;,&quot;requestedAuxClockOutputFrequency_Hz&quot;:5.0E8,&quot;afvcoDivider&quot;:&quot;2&quot;},&quot;canfdClock&quot;:{&quot;canfdClockSource&quot;:&quot;FPLLO&quot;}}}},&quot;module39&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-uart-protocol-upb&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;uart_protocol_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;uart_protocol_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;UART1&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module1&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/dspic33-configuration-bits&quot;,&quot;imports&quot;:{&quot;dspic33_configuration_bits&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;dspic33_configuration_bits&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;Configuration Bits&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module0&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/main-16bit-manager&quot;,&quot;imports&quot;:{&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;main&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;main-16bit-manager&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;MAIN MANAGER&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module3&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-pin-manager&quot;,&quot;imports&quot;:{&quot;pic24-dspic33-pin-manager&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pic24-dspic33-pin-manager&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;Pin Manager&quot;}},&quot;device-meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;interrupt-16bit-interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}},&quot;system-16bit-initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;adapterdata&quot;:{&quot;pps&quot;:{&quot;data&quot;:{&quot;UART&quot;:{&quot;U1RX&quot;:&quot;RD4&quot;},&quot;UART1&quot;:{&quot;U1RX&quot;:&quot;RD4&quot;},&quot;CAN&quot;:{&quot;CAN1RX&quot;:&quot;RD6&quot;},&quot;CAN1&quot;:{&quot;CAN1RX&quot;:&quot;RD6&quot;},&quot;CLC&quot;:{&quot;CLCINC&quot;:&quot;&quot;},&quot;CLC1&quot;:{&quot;CLCINC&quot;:&quot;&quot;}},&quot;users&quot;:{&quot;module39&quot;:{&quot;mod_name&quot;:&quot;UART1&quot;},&quot;module7&quot;:{&quot;mod_name&quot;:&quot;CAN1&quot;},&quot;module12&quot;:{&quot;mod_name&quot;:&quot;CLC1&quot;}}},&quot;cname&quot;:{&quot;eview&quot;:{&quot;dataMap&quot;:{&quot;RD7&quot;:{&quot;value&quot;:&quot;LED_GREEN&quot;},&quot;RC10&quot;:{&quot;value&quot;:&quot;GPIO_1&quot;},&quot;RC11&quot;:{&quot;value&quot;:&quot;GPIO_2&quot;},&quot;RD12&quot;:{&quot;value&quot;:&quot;TP_PIM&quot;},&quot;RD15&quot;:{&quot;value&quot;:&quot;LED_DP_PIM&quot;},&quot;RD8&quot;:{&quot;value&quot;:&quot;LED_RED&quot;},&quot;RD9&quot;:{&quot;value&quot;:&quot;FAULT&quot;},&quot;RC14&quot;:{&quot;value&quot;:&quot;DPD_TP31&quot;}}}},&quot;high&quot;:{&quot;eview&quot;:{&quot;dataMap&quot;:{&quot;RD9&quot;:{&quot;value&quot;:true}}}},&quot;odc&quot;:{&quot;eview&quot;:{&quot;dataMap&quot;:{&quot;RD9&quot;:{&quot;value&quot;:true}}}}}}},&quot;module2&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-interrupt&quot;,&quot;imports&quot;:{&quot;int_16bit_core_v3&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;int_16bit_core_v3&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;INTERRUPT CORE&quot;}},&quot;config_bit&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;config-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module1&quot;,&quot;exportId&quot;:&quot;config_16bit_interface&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;contextAltRegSet1&quot;:&quot;IPL6&quot;,&quot;intTable&quot;:[{&quot;rowId&quot;:54.0,&quot;uid&quot;:&quot;dynamicRow_module23_CCT1&quot;,&quot;priority&quot;:&quot;5&quot;},{&quot;rowId&quot;:59.0,&quot;uid&quot;:&quot;dynamicRow_module23_CCP1&quot;,&quot;priority&quot;:&quot;1&quot;},{&quot;rowId&quot;:32.0,&quot;uid&quot;:&quot;dynamicRow_module34_CMP3&quot;,&quot;priority&quot;:&quot;6&quot;},{&quot;rowId&quot;:33.0,&quot;uid&quot;:&quot;dynamicRow_module36_CMP1&quot;,&quot;priority&quot;:&quot;6&quot;},{&quot;rowId&quot;:24.0,&quot;uid&quot;:&quot;dynamicRow_module43_ADCAN0&quot;,&quot;priority&quot;:&quot;1&quot;},{&quot;rowId&quot;:57.0,&quot;uid&quot;:&quot;dynamicRow_module20_T1&quot;,&quot;priority&quot;:&quot;3&quot;},{&quot;rowId&quot;:5.0,&quot;uid&quot;:&quot;dynamicRow_module43_ADCAN19&quot;,&quot;priority&quot;:&quot;1&quot;},{&quot;rowId&quot;:11.0,&quot;uid&quot;:&quot;dynamicRow_module43_ADCAN1&quot;,&quot;priority&quot;:&quot;1&quot;}],&quot;contextAltRegSet2&quot;:&quot;IPL5&quot;,&quot;contextAltRegSet3&quot;:&quot;OFF&quot;}}}},&quot;module107&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/cmp-dac-driver&quot;,&quot;imports&quot;:{&quot;cmp_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;cmp-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module36&quot;,&quot;exportId&quot;:&quot;cmp_interface&quot;,&quot;label&quot;:&quot;CMP1&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[&quot;cmp_interface&quot;]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;nonInvertingInput&quot;:&quot;CMP1B&quot;,&quot;customName&quot;:&quot;CMP_ISEC_SC&quot;,&quot;comparatorHysteresisSelect&quot;:&quot;None&quot;,&quot;interruptEvent&quot;:&quot;Interrupts are disabled&quot;,&quot;digitalFilterEnable&quot;:true}}}},&quot;module31&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-wdt-upb-v1&quot;,&quot;imports&quot;:{&quot;wdt_upb_16bit_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;wdt_upb_16bit_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;WATCHDOG&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;config_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;config-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module1&quot;,&quot;exportId&quot;:&quot;config_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module109&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/crc-16bit-driver&quot;,&quot;imports&quot;:{&quot;crc_basic&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;crc-basic&quot;,&quot;version&quot;:&quot;^1.0.2&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module33&quot;,&quot;exportId&quot;:&quot;crc_basic&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;polynomial&quot;:{&quot;preDefinedPolynomial&quot;:&quot;CRC-16&quot;},&quot;data&quot;:{&quot;crcData&quot;:&quot;16&quot;},&quot;crcSimulator&quot;:{&quot;reverseCrcValue&quot;:true}}}},&quot;module36&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-cmp-dac&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;dac_pdm_nbit_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;dac_pdm_nbit_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;CMP1&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;hardware&quot;:{&quot;clkdivDacctrl1l&quot;:&quot;1:4&quot;,&quot;fclkdivDacctrl1l&quot;:&quot;1:8&quot;}}}},&quot;module79&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/icd-16bit-driver&quot;,&quot;imports&quot;:{&quot;icd_v7&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;icd_v7&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;ICD&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;config_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;config-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module1&quot;,&quot;exportId&quot;:&quot;config_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;emulatorPinPlacement&quot;:&quot;Communicate on PGC2 and PGD2&quot;}}}},&quot;module104&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/cmp-dac-driver&quot;,&quot;imports&quot;:{&quot;cmp_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;cmp-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module34&quot;,&quot;exportId&quot;:&quot;cmp_interface&quot;,&quot;label&quot;:&quot;CMP3&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[&quot;cmp_interface&quot;]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;nonInvertingInput&quot;:&quot;CMP3B&quot;,&quot;customName&quot;:&quot;CMP_IPRI_SC&quot;,&quot;comparatorHysteresisSelect&quot;:&quot;None&quot;,&quot;interruptEvent&quot;:&quot;Interrupts are disabled&quot;,&quot;digitalFilterEnable&quot;:true}}}},&quot;module35&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-cmp-dac&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;dac_pdm_nbit_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;dac_pdm_nbit_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;CMP2&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module34&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-cmp-dac&quot;,&quot;imports&quot;:{&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;clock_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;clock-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module5&quot;,&quot;exportId&quot;:&quot;clock_16bit_interface&quot;}},&quot;dac_pdm_nbit_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;dac_pdm_nbit_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;CMP3&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;hardware&quot;:{&quot;clkdivDacctrl1l&quot;:&quot;1:4&quot;,&quot;fclkdivDacctrl1l&quot;:&quot;1:8&quot;}}}},&quot;module12&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-cla-clc-upb&quot;,&quot;imports&quot;:{&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;pin_standard&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pin-standard&quot;,&quot;version&quot;:&quot;^0.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module4&quot;,&quot;exportId&quot;:&quot;pin-standard&quot;}},&quot;cla_clc_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;cla_clc_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;CLC1&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module33&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-crc-upb&quot;,&quot;imports&quot;:{&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}},&quot;math_progcrc_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;math_progcrc_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;CRC&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module128&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/cmp-dac-driver&quot;,&quot;imports&quot;:{&quot;cmp_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;cmp-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module35&quot;,&quot;exportId&quot;:&quot;cmp_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;customName&quot;:&quot;DAC_DEBUG&quot;},&quot;modeSettings&quot;:{&quot;dacOutputEnable&quot;:true,&quot;dacDataHigh&quot;:205.0}}}},&quot;module90&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pwm-hs-driver&quot;,&quot;imports&quot;:{&quot;pwm_hs_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pwm-hs-interface&quot;,&quot;version&quot;:&quot;^2.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module44&quot;,&quot;exportId&quot;:&quot;pwm_motor_control&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;pwmMasterSetting&quot;:{&quot;masterReqFrequency&quot;:{&quot;value&quot;:230.0,&quot;unit&quot;:&quot;kHz&quot;},&quot;masterDutyCycle&quot;:0.0,&quot;masterEnableHighResolution&quot;:true,&quot;masterOperationMode&quot;:&quot;Independent Edge&quot;},&quot;PWM Generator 1&quot;:{&quot;genRequestedFrequency1&quot;:{&quot;value&quot;:230.0,&quot;unit&quot;:&quot;kHz&quot;},&quot;genEnableHighResolution1&quot;:true,&quot;genDutyCycle1&quot;:0.0,&quot;genOperationMode1&quot;:&quot;Independent Edge&quot;,&quot;genDeadTimeLow1&quot;:{&quot;value&quot;:150.0,&quot;unit&quot;:&quot;ns&quot;},&quot;genDeadTimeHigh1&quot;:{&quot;value&quot;:150.0,&quot;unit&quot;:&quot;ns&quot;},&quot;dataUpdateSettings1&quot;:&quot;Client SOC&quot;,&quot;updateTrigger1&quot;:&quot;Trigger A&quot;,&quot;triggerOutputSelection1&quot;:&quot;Trigger C compare event&quot;,&quot;adcTriggerGen1&quot;:[{&quot;rowId&quot;:0.0,&quot;uid&quot;:&quot;defaultRow_0&quot;,&quot;triggerCComp&quot;:false,&quot;triggerAComp&quot;:true,&quot;triggerBComp&quot;:false},{&quot;rowId&quot;:2.0,&quot;uid&quot;:&quot;defaultRow_1&quot;,&quot;triggerBComp&quot;:false,&quot;triggerAComp&quot;:true}],&quot;masterUpdateEnable1&quot;:true,&quot;startOfCycleTrigger1&quot;:&quot;Self-trigger&quot;,&quot;genFaultInputSource1&quot;:&quot;CLC1 output&quot;,&quot;genFaultInputPolarity1&quot;:&quot;Active-high&quot;,&quot;genCustomName1&quot;:&quot;PWM_PRI_1&quot;,&quot;genPWMLowOverride1&quot;:&quot;disabled&quot;},&quot;PWM Generator 2&quot;:{&quot;useGenerator2&quot;:true,&quot;genRequestedFrequency2&quot;:{&quot;value&quot;:230.0,&quot;unit&quot;:&quot;kHz&quot;},&quot;genDutyCycle2&quot;:0.0,&quot;genEnableHighResolution2&quot;:true,&quot;genOperationMode2&quot;:&quot;Independent Edge&quot;,&quot;genDeadTimeLow2&quot;:{&quot;value&quot;:150.0,&quot;unit&quot;:&quot;ns&quot;},&quot;genDeadTimeHigh2&quot;:{&quot;value&quot;:150.0,&quot;unit&quot;:&quot;ns&quot;},&quot;dataUpdateSettings2&quot;:&quot;Client SOC&quot;,&quot;updateTrigger2&quot;:&quot;Trigger A&quot;,&quot;triggerOutputSelection2&quot;:&quot;Trigger C compare event&quot;,&quot;startOfCycleTrigger2&quot;:&quot;Trigger output selected by PG1 or PG5&quot;,&quot;genFaultInputSource2&quot;:&quot;CLC1 output&quot;,&quot;genFaultInputPolarity2&quot;:&quot;Active-high&quot;,&quot;genCustomName2&quot;:&quot;PWM_SEC_1&quot;},&quot;PWM Generator 3&quot;:{&quot;useGenerator3&quot;:true,&quot;genEnableHighResolution3&quot;:true,&quot;genDutyCycle3&quot;:0.0,&quot;genRequestedFrequency3&quot;:{&quot;value&quot;:230.0,&quot;unit&quot;:&quot;kHz&quot;},&quot;genOperationMode3&quot;:&quot;Independent Edge&quot;,&quot;genDeadTimeLow3&quot;:{&quot;value&quot;:150.0,&quot;unit&quot;:&quot;ns&quot;},&quot;genDeadTimeHigh3&quot;:{&quot;value&quot;:150.0,&quot;unit&quot;:&quot;ns&quot;},&quot;dataUpdateSettings3&quot;:&quot;Client SOC&quot;,&quot;startOfCycleTrigger3&quot;:&quot;Trigger output selected by PG2 or PG6&quot;,&quot;triggerOutputSelection3&quot;:&quot;Trigger C compare event&quot;,&quot;adcTriggerGen3&quot;:[{&quot;rowId&quot;:0.0,&quot;uid&quot;:&quot;defaultRow_0&quot;,&quot;triggerAComp&quot;:false}],&quot;genFaultInputSource3&quot;:&quot;CLC1 output&quot;,&quot;genFaultInputPolarity3&quot;:&quot;Active-high&quot;,&quot;genCustomName3&quot;:&quot;PWM_PRI_2&quot;},&quot;PWM Generator 4&quot;:{&quot;useGenerator4&quot;:true,&quot;genEnableHighResolution4&quot;:true,&quot;genRequestedFrequency4&quot;:{&quot;value&quot;:230.0,&quot;unit&quot;:&quot;kHz&quot;},&quot;genDutyCycle4&quot;:0.0,&quot;genOperationMode4&quot;:&quot;Independent Edge&quot;,&quot;genDeadTimeLow4&quot;:{&quot;value&quot;:150.0,&quot;unit&quot;:&quot;ns&quot;},&quot;genDeadTimeHigh4&quot;:{&quot;value&quot;:150.0,&quot;unit&quot;:&quot;ns&quot;},&quot;dataUpdateSettings4&quot;:&quot;SOC&quot;,&quot;adcTriggerGen4&quot;:[{&quot;rowId&quot;:0.0,&quot;uid&quot;:&quot;defaultRow_0&quot;,&quot;triggerAComp&quot;:false}],&quot;startOfCycleTrigger4&quot;:&quot;Trigger output selected by PG3 or PG7&quot;,&quot;triggerOutputSelection4&quot;:&quot;Trigger C compare event&quot;,&quot;masterUpdateEnable4&quot;:true,&quot;updateTrigger4&quot;:&quot;Manual&quot;,&quot;genFaultInputSource4&quot;:&quot;CLC1 output&quot;,&quot;genFaultInputPolarity4&quot;:&quot;Active-high&quot;,&quot;genCustomName4&quot;:&quot;PWM_SEC_2&quot;},&quot;PWM Generator 6&quot;:{&quot;useGenerator6&quot;:false,&quot;genCustomName6&quot;:&quot;PWM_LEB&quot;,&quot;genEnableHighResolution6&quot;:false,&quot;genOperationMode6&quot;:&quot;Independent Edge&quot;,&quot;genRequestedFrequency6&quot;:{&quot;value&quot;:10.0,&quot;unit&quot;:&quot;kHz&quot;},&quot;genDutyCycle6&quot;:0.1,&quot;dataUpdateSettings6&quot;:&quot;SOC&quot;,&quot;genPWMLowOverride6&quot;:&quot;disabled&quot;,&quot;genPwmHighOverride6&quot;:&quot;disabled&quot;,&quot;startOfCycleTrigger6&quot;:&quot;Self-trigger&quot;,&quot;genEnablePWM6&quot;:false,&quot;masterUpdateEnable6&quot;:true}}}},&quot;module102&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pwm-driver&quot;,&quot;imports&quot;:{&quot;pwm_generator&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;pwm-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module25&quot;,&quot;exportId&quot;:&quot;basic_ccp&quot;,&quot;label&quot;:&quot;SCCP3&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[&quot;pwm_generator&quot;]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;customName&quot;:&quot;FAN_PWM&quot;},&quot;configurationSettings&quot;:{&quot;pwmFrequency&quot;:20000.0,&quot;dutyCycle&quot;:0.0}}}},&quot;module50&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/pic24-dspic33-dmt-upb&quot;,&quot;imports&quot;:{&quot;wdt_dmt_upb_v1&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;wdt_dmt_upb_v1&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;DMT&quot;}},&quot;system_16bit_initializer&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;system-16bit-initializer&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module0&quot;,&quot;exportId&quot;:&quot;system_16bit_initializer&quot;}},&quot;interrupt_service&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;interrupt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module2&quot;,&quot;exportId&quot;:&quot;interrupt_16bit_interface&quot;}},&quot;config_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;config-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module1&quot;,&quot;exportId&quot;:&quot;config_16bit_interface&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{}},&quot;module94&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/adc-multicore-driver&quot;,&quot;imports&quot;:{&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;adc_multicore&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;adc-multicore&quot;,&quot;version&quot;:&quot;^2.1.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module43&quot;,&quot;exportId&quot;:&quot;adc_multicore&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;Dedicated Core0 Settings&quot;:{&quot;useCore0&quot;:true,&quot;Core0&quot;:[{&quot;rowId&quot;:0.0,&quot;uid&quot;:&quot;dynamicRow_AN0&quot;,&quot;channelEnable&quot;:true,&quot;trigger&quot;:&quot;Common Software Trigger&quot;,&quot;customName&quot;:&quot;ISEC_CT&quot;,&quot;interrupt&quot;:false}],&quot;requestedCore0SamplingTime&quot;:0.04},&quot;Dedicated Core1 Settings&quot;:{&quot;useCore1&quot;:true,&quot;Core1&quot;:[{&quot;rowId&quot;:0.0,&quot;uid&quot;:&quot;dynamicRow_AN1&quot;,&quot;channelEnable&quot;:true,&quot;trigger&quot;:&quot;Common Software Trigger&quot;,&quot;customName&quot;:&quot;ISEC_AVG&quot;,&quot;channelName&quot;:&quot;ANA1&quot;,&quot;interrupt&quot;:false}],&quot;requestedCore1SamplingTime&quot;:0.04},&quot;sharedCore&quot;:{&quot;adcTable&quot;:[{&quot;rowId&quot;:0.0,&quot;uid&quot;:&quot;dynamicRow_AN2&quot;,&quot;channelEnable&quot;:true,&quot;customName&quot;:&quot;VSEC&quot;,&quot;trigger&quot;:&quot;Common Software Trigger&quot;},{&quot;rowId&quot;:5.0,&quot;uid&quot;:&quot;dynamicRow_AN7&quot;,&quot;channelEnable&quot;:true,&quot;customName&quot;:&quot;IPRI_CT&quot;,&quot;trigger&quot;:&quot;Common Software Trigger&quot;},{&quot;rowId&quot;:8.0,&quot;uid&quot;:&quot;dynamicRow_AN10&quot;,&quot;channelEnable&quot;:true,&quot;customName&quot;:&quot;VPRI&quot;,&quot;trigger&quot;:&quot;Common Software Trigger&quot;},{&quot;rowId&quot;:12.0,&quot;uid&quot;:&quot;dynamicRow_AN14&quot;,&quot;channelEnable&quot;:true,&quot;customName&quot;:&quot;TEMP&quot;,&quot;trigger&quot;:&quot;Common Software Trigger&quot;},{&quot;rowId&quot;:17.0,&quot;uid&quot;:&quot;dynamicRow_AN19&quot;,&quot;channelEnable&quot;:true,&quot;customName&quot;:&quot;VRAIL_5V&quot;,&quot;trigger&quot;:&quot;Common Software Trigger&quot;,&quot;interrupt&quot;:false}],&quot;requestedSharedCoreSamplingTime&quot;:0.04},&quot;software&quot;:{&quot;interruptDriven&quot;:false}}}},&quot;module71&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/wdt-16bit-driver&quot;,&quot;imports&quot;:{&quot;wdt_16bit_interface&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;wdt-16bit-interface&quot;,&quot;version&quot;:&quot;^1.0.1&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module31&quot;,&quot;exportId&quot;:&quot;wdt_16bit_interface&quot;}},&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;wdtMode&quot;:&quot;Non-Window mode&quot;}}}},&quot;module70&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/timer&quot;,&quot;imports&quot;:{&quot;timer_periodic&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;timer-periodic&quot;,&quot;version&quot;:&quot;^2.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module20&quot;,&quot;exportId&quot;:&quot;timer_periodic&quot;,&quot;label&quot;:&quot;TMR1&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[&quot;timer_periodic&quot;]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;interruptDriven&quot;:true,&quot;requestedTimerPeriod&quot;:{&quot;value&quot;:100.0,&quot;unit&quot;:&quot;us&quot;}}}}},&quot;module92&quot;:{&quot;scriptId&quot;:&quot;@mchp-mcc/uart-driver&quot;,&quot;imports&quot;:{&quot;device_meta&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;device-meta&quot;,&quot;version&quot;:&quot;^1.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;mccDevice&quot;,&quot;exportId&quot;:&quot;meta&quot;}},&quot;uart_basic&quot;:{&quot;interfaceId&quot;:{&quot;name&quot;:&quot;uart-basic&quot;,&quot;version&quot;:&quot;^6.0.0&quot;},&quot;handle&quot;:{&quot;providerId&quot;:&quot;module39&quot;,&quot;exportId&quot;:&quot;uart_basic&quot;,&quot;label&quot;:&quot;UART1&quot;}}},&quot;framewSpecificState&quot;:{&quot;userEditedImports&quot;:[&quot;uart_basic&quot;]},&quot;payload&quot;:{&quot;main&quot;:{&quot;software&quot;:{&quot;baudrate&quot;:115200.0}}}}},&quot;content&quot;:{&quot;@mchp-mcc/pic-16bit&quot;:&quot;5.11.4&quot;,&quot;@mchp-mcc/pwm-hs-driver&quot;:&quot;2.2.1&quot;,&quot;@mchp-mcc/clock-16bit-driver&quot;:&quot;1.2.1&quot;,&quot;@mchp-mcc/pic24-dspic33-dmt-upb&quot;:&quot;1.1.1&quot;,&quot;@mchp-mcc/pic24-dspic33-clock-sib&quot;:&quot;1.4.2&quot;,&quot;@mchp-mcc/dmt-16bit-driver&quot;:&quot;1.0.6&quot;,&quot;@mchp-mcc/timer&quot;:&quot;1.2.1&quot;,&quot;@mchp-mcc/crc-16bit-driver&quot;:&quot;1.0.3&quot;,&quot;@mchp-mcc/main-16bit-manager&quot;:&quot;1.1.2&quot;,&quot;@mchp-mcc/dspic33-configuration-bits&quot;:&quot;1.2.2&quot;,&quot;@mchp-mcc/pin-content-processor&quot;:&quot;3.8.0&quot;,&quot;@mchp-mcc/pic24-dspic33-wdt-upb-v1&quot;:&quot;1.2.1&quot;,&quot;@mchp-mcc/icd-16bit-driver&quot;:&quot;1.0.3&quot;,&quot;@mchp-mcc/pic24-dspic33-interrupt&quot;:&quot;1.3.1&quot;,&quot;@mchp-mcc/pic24-dspic33-mccp-upb&quot;:&quot;1.6.4&quot;,&quot;@mchp-mcc/cmp-dac-driver&quot;:&quot;1.0.5&quot;,&quot;@mchp-mcc/can-fd-driver&quot;:&quot;1.2.2&quot;,&quot;@mchp-mcc/pic24-dspic33-pin-manager&quot;:&quot;1.3.0&quot;,&quot;@mchp-mcc/pwm-driver&quot;:&quot;1.0.5&quot;,&quot;@mchp-mcc/wdt-16bit-driver&quot;:&quot;1.0.8&quot;,&quot;@mchp-mcc/pic24-dspic33-reset&quot;:&quot;1.1.0&quot;,&quot;@mchp-mcc/pic24-dspic33-pwm-pc-upb&quot;:&quot;2.4.2&quot;,&quot;@mchp-mcc/pic24-dspic33-adc-multicore&quot;:&quot;2.4.3&quot;,&quot;@mchp-mcc/pic24-dspic33-can-fd-upb&quot;:&quot;1.7.0&quot;,&quot;@mchp-mcc/clc-16bit-driver&quot;:&quot;1.0.6-dev.1&quot;,&quot;@mchp-mcc/adc-multicore-driver&quot;:&quot;2.1.4&quot;,&quot;@mchp-mcc/pic24-dspic33-tmr-class-upb&quot;:&quot;1.5.3&quot;,&quot;@mchp-mcc/uart-driver&quot;:&quot;1.10.1&quot;,&quot;@mchp-mcc/pic24-dspic33-cla-clc-upb&quot;:&quot;1.3.0&quot;,&quot;@mchp-mcc/pic24-dspic33-uart-protocol-upb&quot;:&quot;1.5.0&quot;,&quot;@mchp-mcc/pic24-dspic33-crc-upb&quot;:&quot;1.3.0&quot;,&quot;@mchp-mcc/pic24-dspic33-cmp-dac&quot;:&quot;1.4.2&quot;}}</value>
      </entry>
   </tokenMap>
   <generatedFileHashHistoryMap class="java.util.TreeMap">
      <entry>
         <file>main.c</file>
         <hash>edd6be2b78c67a30daaab2db2957fd761d3332068cbb448d2995d4a42382680f</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc\adc1.h</file>
         <hash>d62ab70660af1995b1bdadfa1f80696ef0c98bf1693889e9836bef96df6a5aea</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc\adc_features.h</file>
         <hash>b79f5b1b4e098c2f1852568f54d3f8f2128dc7c425eb3075191470bdb43a6a8e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc\adc_interface.h</file>
         <hash>53bfec1b839f003cf3a85c68b4580fa00190dba81f201754aaa09cb79da13673</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc\adc_types.h</file>
         <hash>9005e3766ebb9c3ddd198dbe281f72572e0057b0c0ee663e1e11536bf4e75d49</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\adc\src\adc1.c</file>
         <hash>647b1ef6ff16b2b0d08e86bb8c55695c420b27dbd16e3bba89803253d6774172</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\can\can1.h</file>
         <hash>1e1a7b4005e15c30695865a4dc3572fae3c06f3e5068e0541500e84f14ac109b</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\can\can_features.h</file>
         <hash>7bf66727f70a44f974cafa0ecc616ce9e2e5475461ea030d9c3694461e409b59</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\can\can_interface.h</file>
         <hash>e0f857c5bab592c1f4a241921d01d80657772bfb64212b89dabbd87bbac5df94</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\can\can_types.h</file>
         <hash>3bde3510361d1b8f19b100a2aa1736bd02519934cc3149ff2a8b4cc92d1d8c5f</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\can\src\can1.c</file>
         <hash>fdbfc4e9390d238168134260f996ff1f584ce23e1744ab2c534a68042323ac65</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clc\clc1.h</file>
         <hash>f7ed8d59dab3256fbead1954762ac01318a1d27ee55935bb5f875454d41d5a2e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clc\clc_interface.h</file>
         <hash>701952d56e9a6f3bfaa0ff4727802c82cfd5ff5cd11c27c11a6ab76e46b1190a</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\clc\src\clc1.c</file>
         <hash>bd56b9a4b3f0632fb4d20cfc3d477bd105607b3f0244675e00637f8633705736</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\cmp\cmp1.h</file>
         <hash>c02cef5233c4cce7861503a7250c5467f4572211e3f3e7afd9df7a6f45ed593e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\cmp\cmp2.h</file>
         <hash>c2769c7c578c25368946a15a8afd3354cac8425445fcf3d14c1aef6c9eaa9cae</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\cmp\cmp3.h</file>
         <hash>45ae0004cad5b237f2595e541d27a279b9da520b3c6f566c4459ba43d946e5de</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\cmp\cmp_interface.h</file>
         <hash>bb82176cad6f8bf3ea96cb0b3f9576353d0f7107c51fb9f630577ebd15503d1c</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\cmp\src\cmp1.c</file>
         <hash>8f240de5ba1a01184df1fc5545b46254cf11ce8c869c38f7b405ca0074569d30</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\cmp\src\cmp2.c</file>
         <hash>9281fcf94a53fad04c389c013226350313033a485edba3cffaa999ec6ccf788d</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\cmp\src\cmp3.c</file>
         <hash>932b4ccb8c082a8391693f889daafe10676fcd5c7ac6e241fa8a037f565d8e23</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\crc\crc.h</file>
         <hash>a7dc0c690775022882883386b37ff305b62151aad2fa1666c962450ab886ca7a</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\crc\crc_interface.h</file>
         <hash>682ec7ad5ab462fb7f74ec7736d83c9d63c2a7b2201e03a911ba2e64fa15335b</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\crc\crc_types.h</file>
         <hash>049389d06985075be5eebe5e4375abe7b0860f5fa3ded4656534e6a0e6eeed86</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\crc\src\crc.c</file>
         <hash>a81441728600fc54d7cc29cc37a18443948f8ce96f5a28cf6adb99b0cd9a6bed</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm\pwm_interface.h</file>
         <hash>d15fd47e5c33a0c3d86e57312353a761cd562bb5d181006a29032ae193f01b95</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm\pwm_types.h</file>
         <hash>4d60d6d5fc1cb0319b34d4278bd8f763e9e2c6bbc8a68c61a543d771658edc32</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm\sccp3.h</file>
         <hash>d0e8fde14615de0c2ebe8f981598fab7f1f255bdaf67fcfa151410eee9c01786</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm\src\sccp3.c</file>
         <hash>1642b0378802921b65c5286a95fc51a73126657032ce8fb8e7e49e9f20e27cac</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm_hs\pwm.h</file>
         <hash>209f63035fb448c691ff9cf01013f6191e44aaf4ade65f7f2776a79b4f36f1ba</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm_hs\pwm_features.h</file>
         <hash>0080bfe41816c9bed344e221fe768c41c04c461a4b8eb7e579d0ad9f1efc8fec</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm_hs\pwm_hs_interface.h</file>
         <hash>80f09c5d29cba5b696052761d3892df9fdff4924bae8203e5072fa06c0447983</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm_hs\pwm_hs_types.h</file>
         <hash>ebf4d0bfd85e37891a1a1a56790655ec907f2e8424d0ed01dfc9faf9064ec526</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pwm_hs\src\pwm.c</file>
         <hash>ed00f714fea073d531caff3fa3770e9f14c222227d532ca11ac8367caf35e669</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\clock.h</file>
         <hash>ad2a8dd9b80a1032f8157e4cbf40f3278cc5e18eb31f45e58616f7a1d99761e6</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\dmt.h</file>
         <hash>3d42d0fdd64fc96585135b9c94fe80426a986f375c7ec24a79a4718856dcc3ab</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\interrupt.h</file>
         <hash>001df775c4873aea98547dfea0375bc7b9dbaa227c44468d5e6936f1030fc92f</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\interrupt_types.h</file>
         <hash>d3e542a384d35e30e69e03da72344cea23abc6bb6b61527a87393afeaca08f1a</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\pins.h</file>
         <hash>c1e76bffbe01aa0c99f4093e81562cd9c6fec2c0cc0e7729260f7cdf4737d977</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\reset.h</file>
         <hash>669b7d6a3de821b66e0e3f7c50c156ee3ff285abc8eb1d825add77cb15391bc7</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\reset_types.h</file>
         <hash>56cbc60b800e8ec4a1c1ef9f23923abf4776e800168b76809aab29610470859b</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\clock.c</file>
         <hash>49c4d0a1349d5ee0254c72ec2ce7161ef2a5be845a7b41180181686455da8605</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\config_bits.c</file>
         <hash>e18aa903a49406afe46b1c490f3e72acca9b6cb1daaeb0e5ef9db605833a2a33</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\dmt.c</file>
         <hash>60e3f1ad858f66d0665067420236964784dc5b6841c539422c9dc0d71b29cba9</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\dmt_asm.s</file>
         <hash>1a856353ae6f30b5c2e4be0084b0c5be2e93e4f70066640239c83c4482144ee1</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\interrupt.c</file>
         <hash>211d108ee5a6e211ad1826d7498e4e7edcd8fdf9902be16d101ce111140a6f40</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\pins.c</file>
         <hash>e7b971fd4dfae072aeedd5d122d790c4d5be1fecf739a4bc3ecb1dcc2820e7f6</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\reset.c</file>
         <hash>cf2ecf787e11b85ab905899e23becfb7ea6fc358e865abecb3526d9cb21678c0</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\system.c</file>
         <hash>f60980c517686b9d0089f9cada09bcc90e8764dd6d15e5264f6e42e7b2a02672</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\src\traps.c</file>
         <hash>260448eca18bb83bc06507c8d28ffe7d10cff6e445b2bbb44ee077f80406f62e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\system.h</file>
         <hash>ebcdfb45fa51e9dcafa44d9378a46eca8166335602822d1d75cff5b9f51f6eac</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\system_types.h</file>
         <hash>31a432a60a5e13973039c9028245ac4e8f9c0b3fc7c16d5f1460a8b076a9c327</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\traps.h</file>
         <hash>032dec682ab53d9a317dc7fd163b0163a7355e58b4e1f9485201ba17aa9587b1</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\system\watchdog.h</file>
         <hash>5c6574c88234eab896ec254e70252d35438a8065ce6012ee80149dd26155086a</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\timer\sccp1.h</file>
         <hash>cc98406077432b7ddf1681f3a72088236b9e39a2496f53bde215df7bcc588659</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\timer\src\sccp1.c</file>
         <hash>c5aaa949adfc5adf468a82fc6e10e2ecc1bdcbc4f7490337179bc6b9d3716673</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\timer\src\tmr1.c</file>
         <hash>f8ef95f51fc9e29609d45be07544d2289e79d0d61aded5d47b318c7dd8be0871</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\timer\timer_interface.h</file>
         <hash>c53a0065f79303531dd52f678df1c773db1fcc128da2af9d42442ff8d6b3f6ef</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\timer\tmr1.h</file>
         <hash>323fe51bec929ded084a4326c8237dca897541a69db78669543159066e705855</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart\src\uart1.c</file>
         <hash>7fbf372364b3d3147042eeb4a7ec2f5d38cea6e488b67870431b6e349fca6130</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart\uart1.h</file>
         <hash>d7907bce04b3def03373cdc526aba77021e9a39c1528810b10638985d02d6128</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart\uart_interface.h</file>
         <hash>38082824e3fb8f03248bb8ac43aad2a7c9e1794edddbab55935f99244b2ab626</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart\uart_types.h</file>
         <hash>4669bbd1f9e33a3b753c2b0fc557213e3feb761eff9b10acfeb5bc6193b7fd22</hash>
      </entry>
   </generatedFileHashHistoryMap>
</config>