|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Files | Functions
Traps Driver
MPLABX MCC Melody Code Generator

Traps driver with handler for all types of traps using dsPIC MCUs. More...

Collaboration diagram for Traps Driver:

## Files
file | traps.c
| This is the generated driver source file for TRAPS driver.

## Functions
void | TRAPS_halt_on_error (uint16_t code)
| Stores the trap error code and waits forever. This is a weak attribute function. The user can override and implement the same function without weak attribute.

## Detailed Description

## Function Documentation

## ◆ TRAPS_halt_on_error()

void TRAPS_halt_on_error | ( | uint16_t | code | ) |

Parameters

  [in] | code | - trap error code

Returns
  none

Here is the caller graph for this function: