<map id="MCC_Custom_User_Config" name="MCC_Custom_User_Config">
<area shape="rect" id="Node000001" title="Contains custom peripheral initialization." alt="" coords="5,131,185,157"/>
<area shape="rect" id="Node000002" href="$a00515.html#gac779b9d8bce64e8de686bd78be25ea09" title="Contains PWM initialization that was not supported by MCC generated code." alt="" coords="233,131,416,157"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="185,141,217,141,217,147,185,147"/>
<area shape="rect" id="Node000003" href="$a00515.html#gaaf5d1e32e8b272aa4785219fa041b394" title="Set the data mode of fault PCI." alt="" coords="497,5,653,32"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="339,128,391,85,426,62,463,42,481,34,483,39,465,46,429,66,394,89,342,132"/>
<area shape="rect" id="Node000004" href="$a00515.html#ga30d00d0393fc5b7bef92269fa3662a8f" title="Set PCI fault acceptance criteria." alt="" coords="478,56,672,99"/>
<area shape="poly" id="edge3_Node000002_Node000004" title=" " alt="" coords="377,127,477,100,479,106,378,133"/>
<area shape="rect" id="Node000005" href="$a00515.html#ga3e7243475a0867eddc73f8c453acf105" title="Set TSYNCDIS bit to determine when PWM should stop after a fault occurs." alt="" coords="464,123,685,165"/>
<area shape="poly" id="edge4_Node000002_Node000005" title=" " alt="" coords="416,141,449,141,449,147,416,147"/>
<area shape="rect" id="Node000006" href="$a00515.html#gaab156f2b7ad138cf32e734bbf7145ef4" title="Enable/Disable the PWM instance output swap bit." alt="" coords="487,189,662,232"/>
<area shape="poly" id="edge5_Node000002_Node000006" title=" " alt="" coords="378,155,479,182,477,188,377,161"/>
<area shape="rect" id="Node000007" href="$a00515.html#ga51d53c1db006afc7c11a0ab15f07093d" title="Set source of fault PCI acceptance qualifier." alt="" coords="505,256,644,283"/>
<area shape="poly" id="edge6_Node000002_Node000007" title=" " alt="" coords="342,156,394,199,429,222,465,242,492,252,490,257,463,246,426,226,391,203,339,160"/>
</map>
