|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
mcc_custom_config.c
1
8#include <xc.h>
9#include "driver/mcc_extension/drv_mcc_extension.h"
10#include "driver/mcc_extension/drv_custom_config_pwm.h"
11#include "driver/mcc_extension/drv_custom_config_adc.h"
12#include "pwrctrl/pwrctrl.h"
13
14
24 void MCC_Custom_User_Config (void)
25{
26 // Initialize PWM as re-triggerable for the cascaded PWM scheme
27 // and setup the PWM fault PCI for hardware fault
28 DRV_Config_Custom_PWM();
29
30}
drv_custom_config_adc.h
Contains ADC initialization that was not supported by MCC generated code.
drv_custom_config_pwm.h
Contains PWM initialization that was not supported by MCC generated code.
drv_mcc_extension.h
Contain the peripheral header files with MCC extension code.
MCC_Custom_User_Config
void MCC_Custom_User_Config(void)
Contains custom peripheral initialization.
Definition mcc_custom_config.c:24
DRV_Config_Custom_PWM
static __inline__ void DRV_Config_Custom_PWM(void)
Contains PWM initialization that was not supported by MCC generated code.
Definition drv_custom_config_pwm.h:25