|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
STATUS_FLAGS_s Struct Reference
Power Control » Power Control Data Types

Power converter status flags. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/pwrctrl/pwrctrl_typedef.h>`

Collaboration diagram for STATUS_FLAGS_s:

## Data Fields
union { |
uint16_t value |
}; |  |

## Detailed Description

This data structure is used to indicate when the there is a fault or running power supply.

Definition at line 79 of file pwrctrl_typedef.h.

## Field Documentation

## ◆ [union]

union { ... }

## ◆ FaultActive

unsigned FaultActive

Definition at line 83 of file pwrctrl_typedef.h.

## ◆ notUsed

unsigned notUsed

Definition at line 84 of file pwrctrl_typedef.h.

## ◆ Running

unsigned Running

Definition at line 82 of file pwrctrl_typedef.h.

## ◆ value

uint16_t value

Definition at line 86 of file pwrctrl_typedef.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/pwrctrl/pwrctrl_typedef.h