|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Functions
PBV_DAB_frame_map.h File Reference
Communication Layer » Power Board Visualizer » PBV Data DAB App

app PBV DAB Frame map file Example More...

`#include <xc.h>`
`#include "PBV_interface.h"`
Include dependency graph for PBV_DAB_frame_map.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Functions
void | App_PBV_DAB_Init (void)
| This function initializes the local pbv objects. these objects are then passed on to the app_PBV_init function to initialize the CAN/UART objects.
void | App_PBV_DAB_Task_10ms (void)
| 10ms PBV task to be execution
void | App_PBV_DAB_Task_1s (void)
| 1 second PBV task to be execution
PBV_Datatype_TX_t * | App_PBV_DAB_Get_TX_Log_ptr (void)

## Detailed Description

Author
  M70027

Definition in file PBV_DAB_frame_map.h.

## Function Documentation

## ◆ App_PBV_DAB_Get_TX_Log_ptr()

PBV_Datatype_TX_t * App_PBV_DAB_Get_TX_Log_ptr | ( | void |  | ) |