|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
FAULT_SETTINGS_s Struct Reference

Contains Fault settings. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/fault/fault_typedef.h>`

Collaboration diagram for FAULT_SETTINGS_s:

## Data Fields
uint16_t | FaultDetected
| Fault indication for fault occurrence.
FAULT_t | Object
| Fault Objects.

## Detailed Description

This data structure is utilized to to set-up the fault settings.

Definition at line 39 of file fault_typedef.h.

## Field Documentation

## ◆ FaultDetected

uint16_t FaultDetected

Definition at line 41 of file fault_typedef.h.

## ◆ Object

FAULT_t Object

Definition at line 42 of file fault_typedef.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/fault/fault_typedef.h