<map id="App_PBV_DAB_Task_1s" name="App_PBV_DAB_Task_1s">
<area shape="rect" id="Node000001" title="1 second PBV task to be execution" alt="" coords="5,56,174,83"/>
<area shape="rect" id="Node000002" href="$a00505.html#gab70a27b3aad7113c3983e82413ca5e4f" title="Reinitializes the objects if any parameters( ID, length, etc) are to be changed to the CAN or UART ob..." alt="" coords="253,5,379,32"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="152,53,238,33,240,38,153,58"/>
<area shape="rect" id="Node000003" href="$a00505.html#ga39ed8d2ee366abaf4aa95a424f9108e3" title="This function links the data from application object to the CAN or UART object and &#160;&#160;This function ch..." alt="" coords="248,56,384,83"/>
<area shape="poly" id="edge2_Node000001_Node000003" title=" " alt="" coords="174,67,233,67,233,72,174,72"/>
<area shape="rect" id="Node000004" href="$a00513.html#gac9618e1ca87e77920c94cdfdcc80321a" title="This converts the raw values to temperature celcius as per device lookup table." alt="" coords="222,107,410,149"/>
<area shape="poly" id="edge3_Node000001_Node000004" title=" " alt="" coords="145,81,217,100,216,105,143,86"/>
</map>
