|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Functions | Variables
pwrctrl_dcdt.c File Reference
Power Control » Control Loop Configuration

Contains individual DCDT control loop initialization functions. More...

`#include <xc.h>`
`#include "pwrctrl_dcdt.h"`
Include dependency graph for pwrctrl_dcdt.c:

Go to the source code of this file.

## Functions
int16_t VMC_2p2zACoefficients[2] | __attribute__ ((space(xmemory)))
| Voltage Loop A-coefficient array.
int16_t VMC_2p2zControlHistory[2] | __attribute__ ((space(ymemory), far))
| Voltage Loop Control history.
void | PwrCtrl_VComp_Initialize (void)
| Initialize the Voltage Loop Control.
void | PwrCtrl_IComp_Initialize (void)
| Initialize the Current Loop Control.
void | PwrCtrl_PComp_Initialize (void)
| Initialize the Power Loop Control.
void | PwrCtrl_ResetControlLoopHistories (void)
| Clear the control and error histories of the control loops.

## Variables
SMPS_2P2Z_T | VMC_2p2z
| Data Object of voltage mode control generated by DCDT.
SMPS_2P2Z_T | IMC_2p2z
| Data Object of current mode control.
SMPS_2P2Z_T | PMC_2p2z
| Data Object of power mode control.

## Detailed Description

Generated main.c file from MPLAB Code Configurator

@Company Microchip Technology Inc.

@File Name dev_TPBLPFC_typedef.c

@Summary This is the generated main.c using PIC24 / dsPIC33 / PIC32MM MCUs.

@Description This source file provides main entry point for system initialization and application code development. Generation Information : Product Revision : PIC24 / dsPIC33 / PIC32MM MCUs - 1.170.0 Device : dsPIC33CH512MP506S1 The generated drivers are tested against the following: Compiler : XC16 v1.70 MPLAB : MPLAB X v6.00

<>

Definition in file pwrctrl_dcdt.c.