|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Typedefs | Enumerations | Functions | Variables
fault_comm_interface.c File Reference
Fault Monitor » Fault Configuration

Contains API functions for fault protection. More...

`#include "fault_common.h"`
`#include "pwrctrl/pwrctrl.h"`
Include dependency graph for fault_comm_interface.c:

Go to the source code of this file.

## Typedefs
typedef enum FAULTLOG_FLAGS_e | FAULTLOG_FLAGS_t

## Enumerations
enum | FAULTLOG_FLAGS_e { FLT_VPRI_OVP , FLT_VPRI_UVP , FLT_VSEC_OVP , FLT_VSEC_UVP , FLT_IPRI_OCP , FLT_ISEC_OCP , FLT_ISNS_SCP , FLT_DAB_TEMP , FLT_RAIL_5V , FLT_LOAD_DISCONNECT , RESET }

## Functions
uint16_t | Fault_GetFlags (void)

## Variables
bool | loadDisconnect

## Typedef Documentation

## ◆ FAULTLOG_FLAGS_t

typedef enum FAULTLOG_FLAGS_e FAULTLOG_FLAGS_t

Definition at line 24 of file fault_comm_interface.c.

## Enumeration Type Documentation

## ◆ FAULTLOG_FLAGS_e

enum FAULTLOG_FLAGS_e

Enumerator
FLT_VPRI_OVP |
FLT_VPRI_UVP |
FLT_VSEC_OVP |
FLT_VSEC_UVP |
FLT_IPRI_OCP |
FLT_ISEC_OCP |
FLT_ISNS_SCP |
FLT_DAB_TEMP |
FLT_RAIL_5V |
FLT_LOAD_DISCONNECT |
RESET |

Definition at line 11 of file fault_comm_interface.c.

## Function Documentation

## ◆ Fault_GetFlags()

uint16_t Fault_GetFlags | ( | void |  | ) |

Definition at line 28 of file fault_comm_interface.c.

Here is the caller graph for this function:

## Variable Documentation

## ◆ loadDisconnect

bool loadDisconnect
| extern

Definition at line 28 of file fault.c.