|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
UART_MSG_RX_OBJ Struct Reference
Communication Layer » Power Board Visualizer » UART Communication

UART msg receive object. More...

Collaboration diagram for UART_MSG_RX_OBJ:

## Data Fields
uint8_t | UART_Frame_State
| UART Receive Frame states.
uint8_t | Length_in_Bytes
| UART bytes Received
uint16_t | Protocol_ID
| Received Frame ID.
uint16_t | Offset
| Offset needed to store data in data
uint16_t | CRC
| received CRC
uint8_t | PBV_Header [PBV_HEADER_SIZE]
| recived Header. 5bytes ( SOF + ID + Length)
uint8_t | data [PBV_RCV_DATABUFFER_SIZE]
| data buffer. linked by the calling application. STATIC(64) bytes for now.

## Detailed Description

Definition at line 104 of file PBV_UART.c.

## Field Documentation

## ◆ CRC

uint16_t CRC

Definition at line 110 of file PBV_UART.c.

## ◆ data

uint8_t data[PBV_RCV_DATABUFFER_SIZE]

Definition at line 112 of file PBV_UART.c.

## ◆ Length_in_Bytes

uint8_t Length_in_Bytes

Definition at line 107 of file PBV_UART.c.

## ◆ Offset

uint16_t Offset

Definition at line 109 of file PBV_UART.c.

## ◆ PBV_Header

uint8_t PBV_Header[PBV_HEADER_SIZE]

Definition at line 111 of file PBV_UART.c.

## ◆ Protocol_ID

uint16_t Protocol_ID

Definition at line 108 of file PBV_UART.c.

## ◆ UART_Frame_State

uint8_t UART_Frame_State

Definition at line 106 of file PBV_UART.c.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/comm/PBV_UART.c