|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
PBV_Datatype_RX_t Struct Reference
Communication Layer » Power Board Visualizer » PBV Interface

More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/comm/PBV_interface.h>`

Collaboration diagram for PBV_Datatype_RX_t:

## Data Fields
uint16_t | Length
| Length of received message in Bytes.
uint32_t | PBV_Protcol_ID
| Protocol ID of the received message.
func_p | Callback_Function
| Callback function.
PBV_MESSAGE_RX_STATE_t | PBV_Message_State
| State of the received message.
uint8_t * | Data_Buffer
| Received Data pointer.

## Detailed Description

pbv App RX data type definition structure

Definition at line 89 of file PBV_interface.h.

## Field Documentation

## ◆ Callback_Function

func_p Callback_Function

Definition at line 92 of file PBV_interface.h.

## ◆ Data_Buffer

uint8_t* Data_Buffer

Definition at line 94 of file PBV_interface.h.

## ◆ Length

uint16_t Length

Definition at line 90 of file PBV_interface.h.

## ◆ PBV_Message_State

PBV_MESSAGE_RX_STATE_t PBV_Message_State

Definition at line 93 of file PBV_interface.h.

## ◆ PBV_Protcol_ID

uint32_t PBV_Protcol_ID

Definition at line 91 of file PBV_interface.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/comm/PBV_interface.h