|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Modules
Control Loop
Configuration Layer

Declaration of macros calculating additional parameters for Control Loop. More...

Collaboration diagram for Control Loop:

## Modules
| Conversion Macros
| Conversion macros for user-declarations of Adaptive Gain Modulation parameters.
#define | VPLOOP_ILOOP_EXE_RATIO (uint16_t)(10 / 2)
| ratio of ILOOP /VPLOOP execution [100KHz / 10KHz], the divide 2 is for interleaved VLoop and PLoop
#define | AGC_MINIMUM_VIN_THRESHOLD 160u
| Minimum VIN threshold to activate AGC in [V]
#define | AGC_MINIMUM_ISEC_THRESHOLD 7
| Minimum current threshold to activate AGC in [A].

## Detailed Description

Note
  The Control Loop Declarations only contain user settings and conversion macros.

## Macro Definition Documentation

## ◆ AGC_MINIMUM_ISEC_THRESHOLD

#define AGC_MINIMUM_ISEC_THRESHOLD 7

Definition at line 46 of file config.h.

## ◆ AGC_MINIMUM_VIN_THRESHOLD

#define AGC_MINIMUM_VIN_THRESHOLD 160u

Definition at line 45 of file config.h.

## ◆ VPLOOP_ILOOP_EXE_RATIO

#define VPLOOP_ILOOP_EXE_RATIO (uint16_t)(10 / 2)

Definition at line 44 of file config.h.