|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
APP_PBV_INTF_API_s Struct Reference
Communication Layer » Power Board Visualizer » User Configuration

structure of API function pointers. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/comm/PBV_config.h>`

Collaboration diagram for APP_PBV_INTF_API_s:

## Data Fields
PBV_Intf_Init_t | init
PBV_Intf_Receive_from_GUI_t | rxGui
PBV_Intf_Transmit_to_GUI_t | txGui
PBV_Intf_Transmit_Ascii_to_GUI_t | txGuiAscii
PBV_Intf_Reinit_t | reinit
PBV_Intf_Link_Data_TX_t | linkDataTX
PBV_Intf_Link_Data_RX_t | linkDataRX

## Detailed Description

Definition at line 88 of file PBV_config.h.

## Field Documentation

## ◆ init

PBV_Intf_Init_t init

Definition at line 90 of file PBV_config.h.

## ◆ linkDataRX

PBV_Intf_Link_Data_RX_t linkDataRX

Definition at line 96 of file PBV_config.h.

## ◆ linkDataTX

PBV_Intf_Link_Data_TX_t linkDataTX

Definition at line 95 of file PBV_config.h.

## ◆ reinit

PBV_Intf_Reinit_t reinit

Definition at line 94 of file PBV_config.h.

## ◆ rxGui

PBV_Intf_Receive_from_GUI_t rxGui

Definition at line 91 of file PBV_config.h.

## ◆ txGui

PBV_Intf_Transmit_to_GUI_t txGui

Definition at line 92 of file PBV_config.h.

## ◆ txGuiAscii

PBV_Intf_Transmit_Ascii_to_GUI_t txGuiAscii

Definition at line 93 of file PBV_config.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/comm/PBV_config.h