|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
OS_RESET_RESETCAUSEBITS_t Struct Reference

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/os/os_reset.h>`

Collaboration diagram for OS_RESET_RESETCAUSEBITS_t:

## Data Fields
bool | reset_by_watchdog:1
unsigned | : 5

## Detailed Description

Definition at line 7 of file os_reset.h.

## Field Documentation

## ◆ __pad0__

unsigned __pad0__

Definition at line 10 of file os_reset.h.

## ◆ reset_by_watchdog

bool reset_by_watchdog

Definition at line 9 of file os_reset.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/os/os_reset.h