<map id="CAN1_RX_FIFO_StatusGet" name="CAN1_RX_FIFO_StatusGet">
<area shape="rect" id="Node000001" title="This returns the CAN1 receive FIFO status." alt="" coords="519,56,699,83"/>
<area shape="rect" id="Node000002" href="$a00533.html#ga4fe1df4cd9f0ce122687dcfab0713b5b" title="Reads the received single message object." alt="" coords="306,5,414,32"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="525,55,414,32,415,27,526,50"/>
<area shape="rect" id="Node000004" href="$a00533.html#gac27e97593d8d9bd7787d116910adc40d" title="Returns the number of CAN messages received in all the FIFO." alt="" coords="249,56,471,83"/>
<area shape="poly" id="edge3_Node000001_Node000004" title=" " alt="" coords="504,72,471,72,471,67,504,67"/>
<area shape="rect" id="Node000005" href="$a00533.html#ga2c655a58965fff8578916b59bed47297" title="Reads the received single message object from the CAN1 receive FIFO." alt="" coords="269,107,451,133"/>
<area shape="poly" id="edge5_Node000001_Node000005" title=" " alt="" coords="526,89,430,109,428,103,525,84"/>
<area shape="rect" id="Node000003" href="$a00503.html#ga5fb4f1d3c69d1871c10a2c0a0ad27f8a" title="Checks the queue and if a message is received then links the data pointer to can object." alt="" coords="5,31,201,57"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="292,28,201,37,201,32,291,23"/>
<area shape="poly" id="edge4_Node000004_Node000003" title=" " alt="" coords="233,60,201,56,201,51,234,54"/>
</map>
