|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
DAC_DC_INTERFACE Struct Reference
MPLABX MCC Melody Code Generator » CMP DAC Driver

Structure containing the function pointers of DAC driver in DC mode. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/mcc_generated_files/cmp/cmp_interface.h>`

Collaboration diagram for DAC_DC_INTERFACE:

## Data Fields
void(* | Enable )(void)
| Pointer to CMPx_DACEnable e.g. CMP1_DACEnable.
void(* | Disable )(void)
| Pointer to CMPx_DACDisable e.g. CMP1_DACDisable.
void(* | DataWrite )(size_t value)
| Pointer to CMPx_DACDataWrite e.g. CMP1_DACDataWrite.

## Detailed Description

Definition at line 54 of file cmp_interface.h.

## Field Documentation

## ◆ DataWrite

void(* DataWrite) (size_t value)

Definition at line 62 of file cmp_interface.h.

## ◆ Disable

void(* Disable) (void)

Definition at line 59 of file cmp_interface.h.

## ◆ Enable

void(* Enable) (void)

Definition at line 56 of file cmp_interface.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/mcc_generated_files/cmp/cmp_interface.h