|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
reset.h
1
17/*
18© [2024] Microchip Technology Inc. and its subsidiaries.
19
20 Subject to your compliance with these terms, you may use Microchip
21 software and any derivatives exclusively with Microchip products.
22 You are responsible for complying with 3rd party license terms
23 applicable to your use of 3rd party software (including open source
24 software) that may accompany Microchip software. SOFTWARE IS ?AS IS.?
25 NO WARRANTIES, WHETHER EXPRESS, IMPLIED OR STATUTORY, APPLY TO THIS
26 SOFTWARE, INCLUDING ANY IMPLIED WARRANTIES OF NON-INFRINGEMENT,
27 MERCHANTABILITY, OR FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT
28 WILL MICROCHIP BE LIABLE FOR ANY INDIRECT, SPECIAL, PUNITIVE,
29 INCIDENTAL OR CONSEQUENTIAL LOSS, DAMAGE, COST OR EXPENSE OF ANY
30 KIND WHATSOEVER RELATED TO THE SOFTWARE, HOWEVER CAUSED, EVEN IF
31 MICROCHIP HAS BEEN ADVISED OF THE POSSIBILITY OR THE DAMAGES ARE
32 FORESEEABLE. TO THE FULLEST EXTENT ALLOWED BY LAW, MICROCHIP?S
33 TOTAL LIABILITY ON ALL CLAIMS RELATED TO THE SOFTWARE WILL NOT
34 EXCEED AMOUNT OF FEES, IF ANY, YOU PAID DIRECTLY TO MICROCHIP FOR
35 THIS SOFTWARE.
36*/
37
38#ifndef RESET_H
39#define RESET_H
40
41#include <stdint.h>
42#include "reset_types.h"
43
53uint16_t RESET_CauseGet(void);
54
63 void RESET_CauseHandler(void);
64
71void RESET_CauseClearAll(void);
72
73#endif /* RESET_H */
reset_types.h
This is the generated driver types header file for the RESET driver.
RESET_CauseHandler
void RESET_CauseHandler(void)
It handles the reset cause by clearing the cause register values. This is a weak attribute function....
RESET_CauseGet
uint16_t RESET_CauseGet(void)
Returns the cause of previous reset.
Definition reset.c:158
RESET_CauseClearAll
void RESET_CauseClearAll(void)
Clears the Reset Cause register.
Definition reset.c:198