|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
CONTROLLER_s Struct Reference
Power Control » Power Control Data Types

Stores data related to the control loop properties. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/pwrctrl/pwrctrl_typedef.h>`

Collaboration diagram for CONTROLLER_s:

## Data Fields
int16_t | Reference
| actual reference
uint16_t | Feedback
| coming
uint16_t | Output
| controller output
int16_t | AgcFactor
| Adaptive gain control.
bool | Enable
| Enable control loop.

## Detailed Description

This data structure manages the control loop properties. The "output" is the output of the controller, "reference" is the actual reference currently being used, and "targetReference" is the desirable reference that the control loop should achieved.

Definition at line 118 of file pwrctrl_typedef.h.

## Field Documentation

## ◆ AgcFactor

int16_t AgcFactor

Definition at line 123 of file pwrctrl_typedef.h.

## ◆ Enable

bool Enable

Definition at line 124 of file pwrctrl_typedef.h.

## ◆ Feedback

uint16_t Feedback

Definition at line 121 of file pwrctrl_typedef.h.

## ◆ Output

uint16_t Output

Definition at line 122 of file pwrctrl_typedef.h.

## ◆ Reference

int16_t Reference

Definition at line 120 of file pwrctrl_typedef.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/pwrctrl/pwrctrl_typedef.h