|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Functions | Variables
pwrctrl.c File Reference
Power Control » Power Control Configuration

Contains power control initialization including control loop initialization and start-up initialization, and the power control execution. More...

`#include <xc.h>`
`#include "pwm_hs/pwm_hs_types.h"`
`#include "pwm_hs/pwm.h"`
`#include "config/macros.h"`
`#include "pwrctrl.h"`
`#include "fault/fault.h"`
`#include "dcdt/pwrctrl_dcdt.h"`
Include dependency graph for pwrctrl.c:

Go to the source code of this file.

## Functions
static void | PwrCtrl_StartUpInitialize (void)
| Initialize the StartUp Ramp configuration.
static void | PwrCtrl_ControlLoopInitialize (void)
| Initializes the control loop.
void | PwrCtrl_StateMachine (POWER_CONTROL_t *pcInstance)
| Manages the power control state machine.
void | PwrCtrl_Initialize (void)
| Initialize the power control parameters.
void | PwrCtrl_Execute (void)
| Executes the power control state machine.
void | PwrCtrl_Reset (void)
| Resets the power control properties.

## Variables
POWER_CONTROL_t | dab
| Global data object for a DAB Converter.

## Detailed Description

<>

Definition in file pwrctrl.c.