|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Special Firmware Options
Configuration Layer

Special functions use to enable or disable special firmware options. More...

Collaboration diagram for Special Firmware Options:

#define | PBV_UART 0
| Enable UART interrupts before.
#define | PBV_CANFD 1
| Use CAN communication for PBV.
#define | PERIOD_MODULATION_DEMO false
| Modulates the period; for further development.
#define | DCDC400V_SYSTEM true
| When true, operates the DAB with protection thresholds for 400V output.
#define | DCDC800V_SYSTEM false
| When true, operates the DAB with protection thresholds for 800V output.
#define | ENABLE_VLOOP_AGC false
| This is an optional feature (not needed for battery application)
#define | DAC_DEBUG false
| test values with PIM DAC output
#define | OPEN_LOOP_POTI false
| test the code with Digital Power Development Board; runs in openloop using potentiometer
#define | OPEN_LOOP_PBV false
| use Power Board visualizer to change the parameters in Open loop operation
#define | CURRENT_CALIBRATION false
| Enable current calibration.
#define | VPRI_OPTOCOUPLER_POLARITY false
| false if not inverted; true if inverted

## Detailed Description

Special functions use to enable or disable special firmware options.

## Macro Definition Documentation

## ◆ CURRENT_CALIBRATION

#define CURRENT_CALIBRATION false

Definition at line 191 of file config.h.

## ◆ DAC_DEBUG

#define DAC_DEBUG false

Definition at line 186 of file config.h.

## ◆ DCDC400V_SYSTEM

#define DCDC400V_SYSTEM true

Definition at line 15 of file config.h.

## ◆ DCDC800V_SYSTEM

#define DCDC800V_SYSTEM false

Definition at line 16 of file config.h.

## ◆ ENABLE_VLOOP_AGC

#define ENABLE_VLOOP_AGC false

Definition at line 17 of file config.h.

## ◆ OPEN_LOOP_PBV

#define OPEN_LOOP_PBV false

Definition at line 188 of file config.h.

## ◆ OPEN_LOOP_POTI

#define OPEN_LOOP_POTI false

Definition at line 187 of file config.h.

## ◆ PBV_CANFD

#define PBV_CANFD 1

Definition at line 16 of file comms_config.h.

## ◆ PBV_UART

#define PBV_UART 0

Definition at line 15 of file comms_config.h.

## ◆ PERIOD_MODULATION_DEMO

#define PERIOD_MODULATION_DEMO false

Definition at line 14 of file config.h.

## ◆ VPRI_OPTOCOUPLER_POLARITY

#define VPRI_OPTOCOUPLER_POLARITY false

Definition at line 195 of file config.h.