<map id="PWM_PCI_Fault_AcceptanceCriteria" name="PWM_PCI_Fault_AcceptanceCriteria">
<area shape="rect" id="Node000001" title="Set PCI fault acceptance criteria." alt="" coords="464,5,658,48"/>
<area shape="rect" id="Node000002" href="$a00515.html#gac779b9d8bce64e8de686bd78be25ea09" title="Contains PWM initialization that was not supported by MCC generated code." alt="" coords="233,13,416,40"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="449,29,417,29,417,24,449,24"/>
<area shape="rect" id="Node000003" href="$a00514.html#gafe646acf69be10085d651f4561909f69" title="Contains custom peripheral initialization." alt="" coords="5,13,185,40"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="218,29,185,29,185,24,218,24"/>
</map>
