|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
CAN_MSG_OBJ Struct Reference
MPLABX MCC Melody Code Generator » CAN FD Driver

This data structure used to configure the CAN FD message object. More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/mcc_generated_files/can/can_types.h>`

Collaboration diagram for CAN_MSG_OBJ:

## Data Fields
uint32_t | msgId
struct CAN_MSG_FIELD | field
uint8_t * | data

## Detailed Description

Definition at line 67 of file can_types.h.

## Field Documentation

## ◆ data

uint8_t* data

Pointer to message data

Definition at line 71 of file can_types.h.

## ◆ field

struct CAN_MSG_FIELD field

Defines the CAN_MSG_FIELD CAN TX/RX Message Object Control

Definition at line 70 of file can_types.h.

## ◆ msgId

uint32_t msgId

Set the CAN Message ID

Definition at line 69 of file can_types.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/mcc_generated_files/can/can_types.h