|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Structures
Here are the data structures with brief descriptions:

C ADC_INTERFACE | Structure containing the function pointers of ADC driver
C ADC_MULTICORE | Structure containing the function pointers of ADC driver
C APP_PBV_INTF_API_s | Structure of API function pointers
C AVERAGING_s |
C CAN1 | This defines the object required for the maintenance of the receive FIFO message object
C CAN1_FIFO_INFO |
C CAN_INTERFACE | Structure containing the function pointers of CAN driver
C CAN_MSG_FIELD | This data structure used to configure the message fields. Some of the fields formatType and brs data should match with the CAN FD configuration in Melody MCC user interface
C CAN_MSG_OBJ | This data structure used to configure the CAN FD message object
C CLC_INTERFACE | Structure containing the function pointers of CLC driver
C CMP_INTERFACE | Structure containing the function pointers of CMP driver
C CONTROLLER_s | Stores data related to the control loop properties
C CRC_INTERFACE | Structure containing the function pointers of CRC driver
C CRC_OBJ |
C DAC_DC_INTERFACE | Structure containing the function pointers of DAC driver in DC mode
C dev_iso_voltage_data_t | Custom data type for isolated voltage measurement
C FAN_DATA_s | A custom data type for fan
C FAULT_OBJ_T | The Fault object data structure contains a list of elements/variables that are used to detect/check a fault
C FAULT_s | Collection of faults to be monitored
C FAULT_SETTINGS_s | Contains Fault settings
C FEEDBACK_SETTINGS_s | Publicly accessible data buffer of most recent runtime data values
C iso_voltage |
C OS_RESET_RESETCAUSEBITS_t |
C OS_SYSTIME_t |
C PBV_Datatype_RX_t |
C PBV_Datatype_TX_t |
C POWER_CONTROL_s | Power control API structure
C PWM_HS_INTERFACE | Structure containing the function pointers of PWM driver
C PWM_INTERFACE | Structure containing the function pointers of PWM generator driver
C PWR_CTRL_PROPERTIES_s | Collection of power control properties
C SENSOR_OFFSET_CAL_s | Stores data related to sensor calibration, including data related to sensor offset
C SMPS_2P2Z_T |
C SMPS_3P3Z_T |
C SMPS_Controller_Options_T |
C SMPS_PID_T |
C START_UP_RAMP_s | Stores data related to the ramping up/down of the reference
C STATUS_FLAGS_s | Power converter status flags
C SWITCH_NODE_s | Power converter switch-node specifications
C TEMP_SETTINGS_s | A custom data type for temperature measurement
C TIMER_INTERFACE | Structure containing the function pointers of TIMER driver
C UART_INTERFACE | Structure containing the function pointers of UART driver
C UART_MSG_RX_OBJ | UART msg receive object
C UART_MSG_TX_OBJ | UART msg Transmit object
C XFT_SMPS_2P2Z_T |