|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
UART_MSG_TX_OBJ Struct Reference
Communication Layer » Power Board Visualizer » UART Communication

UART msg Transmit object. More...

Collaboration diagram for UART_MSG_TX_OBJ:

## Data Fields
uint8_t | UART_Frame_State
| UART Transmit Frame states.
uint8_t | Length_in_Bytes
| UART Bytes to be Transmitted.
uint16_t | Protocol_ID
| Frame ID to be appended.
uint16_t | Offset
| Offset needed for data transmission.
uint16_t | CRC
| calculated CRC
uint8_t | PBV_Header [PBV_HEADER_SIZE]
| sent Header. 5bytes ( SOF + ID + Length)
uint8_t * | data
| data buffer. linked by the calling application. STATIC(64) bytes for now.

## Detailed Description

Definition at line 119 of file PBV_UART.c.

## Field Documentation

## ◆ CRC

uint16_t CRC

Definition at line 125 of file PBV_UART.c.

## ◆ data

uint8_t* data

Definition at line 127 of file PBV_UART.c.

## ◆ Length_in_Bytes

uint8_t Length_in_Bytes

Definition at line 122 of file PBV_UART.c.

## ◆ Offset

uint16_t Offset

Definition at line 124 of file PBV_UART.c.

## ◆ PBV_Header

uint8_t PBV_Header[PBV_HEADER_SIZE]

Definition at line 126 of file PBV_UART.c.

## ◆ Protocol_ID

uint16_t Protocol_ID

Definition at line 123 of file PBV_UART.c.

## ◆ UART_Frame_State

uint8_t UART_Frame_State

Definition at line 121 of file PBV_UART.c.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/comm/PBV_UART.c