<map id="DRV_Config_Custom_PWM" name="DRV_Config_Custom_PWM">
<area shape="rect" id="Node000001" title="Contains PWM initialization that was not supported by MCC generated code." alt="" coords="5,131,189,157"/>
<area shape="rect" id="Node000002" href="$a00515.html#gaaf5d1e32e8b272aa4785219fa041b394" title="Set the data mode of fault PCI." alt="" coords="269,5,426,32"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="112,128,164,85,198,62,236,42,254,34,256,39,238,46,201,66,167,89,115,132"/>
<area shape="rect" id="Node000003" href="$a00515.html#ga30d00d0393fc5b7bef92269fa3662a8f" title="Set PCI fault acceptance criteria." alt="" coords="250,56,445,99"/>
<area shape="poly" id="edge2_Node000001_Node000003" title=" " alt="" coords="150,127,250,100,251,106,151,133"/>
<area shape="rect" id="Node000004" href="$a00515.html#ga3e7243475a0867eddc73f8c453acf105" title="Set TSYNCDIS bit to determine when PWM should stop after a fault occurs." alt="" coords="237,123,458,165"/>
<area shape="poly" id="edge3_Node000001_Node000004" title=" " alt="" coords="189,141,222,141,222,147,189,147"/>
<area shape="rect" id="Node000005" href="$a00515.html#gaab156f2b7ad138cf32e734bbf7145ef4" title="Enable/Disable the PWM instance output swap bit." alt="" coords="260,189,435,232"/>
<area shape="poly" id="edge4_Node000001_Node000005" title=" " alt="" coords="151,155,251,182,250,188,150,161"/>
<area shape="rect" id="Node000006" href="$a00515.html#ga51d53c1db006afc7c11a0ab15f07093d" title="Set source of fault PCI acceptance qualifier." alt="" coords="278,256,417,283"/>
<area shape="poly" id="edge5_Node000001_Node000006" title=" " alt="" coords="115,156,167,199,201,222,238,242,265,252,263,257,236,246,198,226,164,203,112,160"/>
</map>
