|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Enumerations
reset_types.h File Reference
MPLABX MCC Melody Code Generator » Reset Driver

This is the generated driver types header file for the RESET driver. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Enumerations
enum | RESET_TYPES { RESET_ERROR_RCON_TRAPR = 1 , RESET_ERROR_RCON_IOPUWR = 2 , RESET_ERROR_RCON_CM = 3 , RESET_ERROR_RCON_WDTO_ISR = 4 }
enum | RESET_MASKS { RESET_MASK_POR = 0x0001 , RESET_MASK_WDTO = 0x0010 , RESET_MASK_SWR = 0x0040 , RESET_MASK_EXTR = 0x0080 , RESET_MASK_CM = 0x0200 , RESET_MASK_IOPUWR = 0x4000 , RESET_MASK_TRAPR = 0x8000 }

## Detailed Description

RESET Generated Driver Types Header File

Definition in file reset_types.h.

## Enumeration Type Documentation

## ◆ RESET_MASKS

enum RESET_MASKS

Enumerator
RESET_MASK_POR | Defines the power ON Reset flag mask location
RESET_MASK_WDTO | Defines the watchdog timeout reset flag mask location
RESET_MASK_SWR | Defines the software reset mask location
RESET_MASK_EXTR | Defines the external reset mask location
RESET_MASK_CM | Defines the configuration mismatch reset mask location
RESET_MASK_IOPUWR | Defines the illegal opcode or uninitialized W access reset mask location
RESET_MASK_TRAPR | Defines the trap reset mask location

Definition at line 59 of file reset_types.h.

## ◆ RESET_TYPES

enum RESET_TYPES

Enumerator
RESET_ERROR_RCON_TRAPR | A Trap Conflict Reset has occurred
RESET_ERROR_RCON_IOPUWR | An illegal opcode detection, an illegal address mode or Uninitialized W register used as an Address Pointer caused a Reset
RESET_ERROR_RCON_CM | A Configuration Mismatch Reset has occurred
RESET_ERROR_RCON_WDTO_ISR | WDT time-out has occurred

Definition at line 46 of file reset_types.h.