<map id="PBV_CAN_Receive_from_GUI" name="PBV_CAN_Receive_from_GUI">
<area shape="rect" id="Node000001" title="Checks the queue and if a message is received then links the data pointer to can object." alt="" coords="5,108,201,135"/>
<area shape="rect" id="Node000002" href="$a00533.html#ga4fe1df4cd9f0ce122687dcfab0713b5b" title="Reads the received single message object." alt="" coords="306,145,414,172"/>
<area shape="poly" id="edge1_Node000001_Node000002" title=" " alt="" coords="200,133,292,146,291,151,199,138"/>
<area shape="rect" id="Node000009" href="$a00533.html#gac27e97593d8d9bd7787d116910adc40d" title="Returns the number of CAN messages received in all the FIFO." alt="" coords="249,69,471,96"/>
<area shape="poly" id="edge8_Node000001_Node000009" title=" " alt="" coords="196,105,252,96,253,101,196,110"/>
<area shape="rect" id="Node000003" href="$a00533.html#ga57b30800d7bd3b3c936f578ca1fd7e32" title="This function get the FIFO user address, message depth and payload size information." alt="" coords="563,56,702,83"/>
<area shape="poly" id="edge2_Node000002_Node000003" title=" " alt="" coords="390,142,449,117,518,92,548,84,549,89,520,97,451,122,392,147"/>
<area shape="rect" id="Node000004" href="$a00533.html#gaa89329ca22f234476d55536c446b70e3" title="This function read the message object from receive FIFO and update to the user &#160;&#160;message object point..." alt="" coords="534,157,730,184"/>
<area shape="poly" id="edge3_Node000002_Node000004" title=" " alt="" coords="414,158,519,163,519,168,414,164"/>
<area shape="rect" id="Node000006" href="$a00533.html#ga0dab5f41a5a5ef032d23c2ba4890a866" title="This function Update the receive FIFO message increment tail position." alt="" coords="522,208,742,235"/>
<area shape="poly" id="edge5_Node000002_Node000006" title=" " alt="" coords="415,169,520,193,555,202,554,207,518,199,413,174"/>
<area shape="rect" id="Node000007" href="$a00533.html#ga224fbf549503a57f5818cc8391105b8f" title="This function is used to clear the CAN1 receive FIFO overflow status bit." alt="" coords="529,259,736,301"/>
<area shape="poly" id="edge6_Node000002_Node000007" title=" " alt="" coords="384,170,444,206,520,244,537,251,535,256,518,249,441,211,381,175"/>
<area shape="rect" id="Node000008" href="$a00533.html#ga4a6437adcdf1917fffef4e7e5761fda1" title="This returns the CAN1 receive FIFO status." alt="" coords="542,107,722,133"/>
<area shape="poly" id="edge7_Node000002_Node000008" title=" " alt="" coords="413,148,527,132,528,137,414,154"/>
<area shape="rect" id="Node000005" href="$a00533.html#ga61d156b0e75424f9b630cef5c424ac13" title="This function get the DLC enum based decimal value." alt="" coords="793,157,971,184"/>
<area shape="poly" id="edge4_Node000004_Node000005" title=" " alt="" coords="731,168,779,168,779,173,731,173"/>
<area shape="poly" id="edge9_Node000009_Node000003" title=" " alt="" coords="471,75,547,71,547,76,472,80"/>
<area shape="poly" id="edge11_Node000009_Node000008" title=" " alt="" coords="462,94,528,103,527,108,462,99"/>
<area shape="rect" id="Node000010" href="$a00533.html#ga5532c9a884cedd0805a011bf8baaabdd" title="This function get the Receiver FIFO message index value." alt="" coords="519,5,745,32"/>
<area shape="poly" id="edge10_Node000009_Node000010" title=" " alt="" coords="416,66,518,41,554,33,555,38,520,47,418,71"/>
</map>
