|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Enumerations
adc_types.h File Reference
MPLABX MCC Melody Code Generator » ADC Multicore Driver

This is the generated driver types header file for the ADC driver. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Enumerations
enum | ADC_CHANNEL { VSEC , IPRI_CT , VPRI , TEMP , VRAIL_5V , ISEC_CT , ISEC_AVG , MAX_CHANNELS = 7 , ADC_MAX_CHANNELS = 7 }
enum | ADC_DEDICATED_CORE { CORE_0 = 0 , ADC_CORE_0 = 0 , CORE_1 = 1 , ADC_CORE_1 = 1 , MAX_DEDICATED_CORES = 2 , ADC_MAX_DEDICATED_CORES = 2 }
enum | ADC_RESOLUTION_TYPE { ADC_6_BIT_RESOLUTION = 0x0 , ADC_8_BIT_RESOLUTION = 0x1 , ADC_10_BIT_RESOLUTION = 0x2 , ADC_12_BIT_RESOLUTION = 0x3 }
enum | ADC_CMP { MAX_CMPS = 0 , ADC_MAX_CMPS = 0 }
enum | ADC_PWM_INSTANCE { ADC_PWM_GENERATOR_8 , ADC_PWM_GENERATOR_7 , ADC_PWM_GENERATOR_6 , ADC_PWM_GENERATOR_5 , ADC_PWM_GENERATOR_4 , ADC_PWM_GENERATOR_3 , ADC_PWM_GENERATOR_2 , ADC_PWM_GENERATOR_1 }
enum | ADC_PWM_TRIGGERS { ADC_PWM_TRIGGER_1 = 1 , ADC_PWM_TRIGGER_2 = 2 }

## Detailed Description

ADC Generated Driver Types Header File

Definition in file adc_types.h.

## Enumeration Type Documentation

## ◆ ADC_CHANNEL

enum ADC_CHANNEL

Enumerator
VSEC | Channel Name:AN2 Assigned to:Shared Channel
IPRI_CT | Channel Name:AN7 Assigned to:Shared Channel
VPRI | Channel Name:AN10 Assigned to:Shared Channel
TEMP | Channel Name:AN14 Assigned to:Shared Channel
VRAIL_5V | Channel Name:AN19 Assigned to:Shared Channel
ISEC_CT | Channel Name:AN0 Assigned to:Dedicated Core0
ISEC_AVG | Channel Name:ANA1 Assigned to:Dedicated Core1
MAX_CHANNELS | MAX_CHANNELS will be removed in future MCC releases. Use ADC_MAX_CHANNELS instead
ADC_MAX_CHANNELS | Maximum number of channels configured by user in MCC Melody User Interface

Definition at line 55 of file adc_types.h.

## ◆ ADC_CMP

enum ADC_CMP

Enumerator
MAX_CMPS | MAX_CMPS will be removed in future MCC releases. Use ADC_MAX_CMPS instead
ADC_MAX_CMPS | Maximum Comparators configured by user in MCC Melody User Interface

Definition at line 107 of file adc_types.h.

## ◆ ADC_DEDICATED_CORE

enum ADC_DEDICATED_CORE

Enumerator
CORE_0 | CORE_0 will be removed in future MCC releases. Use ADC_CORE_0 instead.
ADC_CORE_0 | Core name:ADC_CORE_0
CORE_1 | CORE_1 will be removed in future MCC releases. Use ADC_CORE_1 instead.
ADC_CORE_1 | Core name:ADC_CORE_1
MAX_DEDICATED_CORES | MAX_DEDICATED_CORES will be removed in future MCC releases. Use ADC_MAX_DEDICATED_CORES instead
ADC_MAX_DEDICATED_CORES | Maximum cores configured by user in MCC Melody User Interface

Definition at line 78 of file adc_types.h.

## ◆ ADC_PWM_INSTANCE

enum ADC_PWM_INSTANCE

Enumerator
ADC_PWM_GENERATOR_8 | PWM name:PWM_GENERATOR_8
ADC_PWM_GENERATOR_7 | PWM name:PWM_GENERATOR_7
ADC_PWM_GENERATOR_6 | PWM name:PWM_GENERATOR_6
ADC_PWM_GENERATOR_5 | PWM name:PWM_GENERATOR_5
ADC_PWM_GENERATOR_4 | PWM name:PWM_GENERATOR_4
ADC_PWM_GENERATOR_3 | PWM name:PWM_GENERATOR_3
ADC_PWM_GENERATOR_2 | PWM name:PWM_GENERATOR_2
ADC_PWM_GENERATOR_1 | PWM name:PWM_GENERATOR_1

Definition at line 120 of file adc_types.h.

## ◆ ADC_PWM_TRIGGERS

enum ADC_PWM_TRIGGERS

Enumerator
ADC_PWM_TRIGGER_1 | PWM TRIGGER 1
ADC_PWM_TRIGGER_2 | PWM TRIGGER 2

Definition at line 137 of file adc_types.h.

## ◆ ADC_RESOLUTION_TYPE

enum ADC_RESOLUTION_TYPE

Enumerator
ADC_6_BIT_RESOLUTION | ADC Resolution of 6 bit
ADC_8_BIT_RESOLUTION | ADC Resolution of 8 bit
ADC_10_BIT_RESOLUTION | ADC Resolution of 10 bit
ADC_12_BIT_RESOLUTION | ADC Resolution of 12 bit

Definition at line 93 of file adc_types.h.