|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
SENSOR_OFFSET_CAL_s Struct Reference
Device Layer » Current Sensor Calibration

Stores data related to sensor calibration, including data related to sensor offset. More...

Collaboration diagram for SENSOR_OFFSET_CAL_s:

## Data Fields
uint32_t | Accumulator
| used for sensor offset measurement at startup
uint16_t | MeasurementCounter
| used for sensor offset measurement at startup
uint16_t | Offset
| measured offset
bool | CalibrationComplete
| set to true if the sensor is calibrated
uint16_t | LimitHigh
| upper bound of what offset should be, offset needs to be < limitHigh and > limitLow for sensorCalibrated = true
uint16_t | LimitLow
| low bound of what offset should be

## Detailed Description

This data structure contains the collection of current sensor properties that the user can initialize and monitor.

Definition at line 22 of file dev_current_sensor.c.

## Field Documentation

## ◆ Accumulator

uint32_t Accumulator

Definition at line 24 of file dev_current_sensor.c.

## ◆ CalibrationComplete

bool CalibrationComplete

Definition at line 27 of file dev_current_sensor.c.

## ◆ LimitHigh

uint16_t LimitHigh

Definition at line 28 of file dev_current_sensor.c.

## ◆ LimitLow

uint16_t LimitLow

Definition at line 29 of file dev_current_sensor.c.

## ◆ MeasurementCounter

uint16_t MeasurementCounter

Definition at line 25 of file dev_current_sensor.c.

## ◆ Offset

uint16_t Offset

Definition at line 26 of file dev_current_sensor.c.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/device/dev_current_sensor.c