|  | Dual Active Bridge Development Board (Part-No. ) |
Content |  |  |  |  |  |

Loading...
Searching...
No Matches
Data Fields
PBV_Datatype_TX_t Struct Reference
Communication Layer » Power Board Visualizer » PBV Interface

More...

`#include <C:/MCU16Projects/bitbucket/dspic33ck-power-dcdc-dual-active-bridge-development-platform/dspic33ck-dab.X/sources/comm/PBV_interface.h>`

Collaboration diagram for PBV_Datatype_TX_t:

## Data Fields
uint16_t | Length
| Length of transmitted message in Bytes.
uint32_t | PBV_Protcol_ID
| Protocol ID.
enum PBV_SIGNAL_ASCII_MODE | PBV_Signal_Ascii
| Object will transmit Signals or ASCII.
PBV_MESSAGE_TX_STATE_t | PBV_Message_State
| State of the TX object.
uint8_t * | Data_Buffer
| Pointer to the data to be transmitted.

## Detailed Description

pbv App TX data type definition structure

Definition at line 75 of file PBV_interface.h.

## Field Documentation

## ◆ Data_Buffer

uint8_t* Data_Buffer

Definition at line 80 of file PBV_interface.h.

## ◆ Length

uint16_t Length

Definition at line 76 of file PBV_interface.h.

## ◆ PBV_Message_State

PBV_MESSAGE_TX_STATE_t PBV_Message_State

Definition at line 79 of file PBV_interface.h.

## ◆ PBV_Protcol_ID

uint32_t PBV_Protcol_ID

Definition at line 77 of file PBV_interface.h.

## ◆ PBV_Signal_Ascii

enum PBV_SIGNAL_ASCII_MODE PBV_Signal_Ascii

Definition at line 78 of file PBV_interface.h.

The documentation for this struct was generated from the following file:

- dspic33ck-dab.X/sources/comm/PBV_interface.h