<map id="MPLABX MCC Melody Code Generator" name="MPLABX MCC Melody Code Generator">
<area shape="rect" id="Node000002" href="$a00532.html" title="High&#45;Speed, 12&#45;Bit Multiple SARs Analog&#45;to&#45;Digital Converter driver using dsPIC MCUs." alt="" coords="206,5,347,32"/>
<area shape="rect" id="Node000003" href="$a00533.html" title="CAN FD Driver using dsPIC MCUs." alt="" coords="224,56,329,83"/>
<area shape="rect" id="Node000004" href="$a00534.html" title="Configurable Logic Cell driver allows the user to specify combinations of signals as inputs to a logi..." alt="" coords="235,107,318,133"/>
<area shape="rect" id="Node000015" href="$a00545.html" title="Clock configurator driver for System and Peripheral Clock using dsPIC MCUs." alt="" coords="231,157,322,184"/>
<area shape="rect" id="Node000005" href="$a00535.html" title="High Speed Analog Comparator with Slope Compensation DAC driver using dsPIC MCUs." alt="" coords="218,208,335,235"/>
<area shape="rect" id="Node000019" href="$a00549.html" title="Device Configuration Bits using dsPIC MCUs." alt="" coords="209,259,344,285"/>
<area shape="rect" id="Node000006" href="$a00536.html" title="16&#45;bit Programmable Cyclic Redundancy Check generator using dsPIC MCUs" alt="" coords="234,309,319,336"/>
<area shape="rect" id="Node000009" href="$a00539.html" title="Deadman Timer (DMT) driver using dsPIC MCUs. The functionality is to interrupt the processor in the e..." alt="" coords="234,360,319,387"/>
<area shape="rect" id="Node000010" href="$a00540.html" title="Interrupt Priority configuration driver using dsPIC MCUs." alt="" coords="224,411,329,437"/>
<area shape="rect" id="Node000001" title="Contains all the module generated by MCC for this application." alt="" coords="5,428,158,471"/>
<area shape="rect" id="Node000012" href="$a00542.html" title="The Pin Driver directs the operation and function of the selected device pins using dsPIC MCUs." alt="" coords="235,461,318,488"/>
<area shape="rect" id="Node000007" href="$a00537.html" title="Pulse Width Modulation Driver using dsPIC MCUs." alt="" coords="231,512,322,539"/>
<area shape="rect" id="Node000008" href="$a00538.html" title="High&#45;Resolution Pulse&#45;Width Modulated (PWM) with Fine Edge Placement using dsPIC MCUs." alt="" coords="220,563,333,589"/>
<area shape="rect" id="Node000014" href="$a00544.html" title="Reset driver using dsPIC MCUs." alt="" coords="231,613,322,640"/>
<area shape="rect" id="Node000013" href="$a00543.html" title="System driver using dsPIC MCUs." alt="" coords="225,664,328,691"/>
<area shape="rect" id="Node000017" href="$a00547.html" title="Timer Driver is a 16&#45;bit timer or 32&#45;bit timer that can operate as a free&#45;running interval timer usin..." alt="" coords="232,715,321,741"/>
<area shape="rect" id="Node000016" href="$a00546.html" title="Traps driver with handler for all types of traps using dsPIC MCUs." alt="" coords="232,765,321,792"/>
<area shape="rect" id="Node000018" href="$a00548.html" title="Universal Asynchronous Receiver Transmitter driver using dsPIC MCUs." alt="" coords="231,816,322,843"/>
<area shape="rect" id="Node000011" href="$a00541.html" title="Watchdog Timer Driver using dsPIC MCUs." alt="" coords="233,867,320,893"/>
</map>
