BSL430.NET 1.2.1

Public Attributes | List of all members
FTD2XX_NET.FTDI.FT_DRIVE_CURRENT Class Reference

Valid values for drive current options on FT2232H, FT4232H and FT232H devices. More...

## Public Attributes
const byte | FT_DRIVE_CURRENT_4MA = 4
| 4mA drive current More...
const byte | FT_DRIVE_CURRENT_8MA = 8
| 8mA drive current More...
const byte | FT_DRIVE_CURRENT_12MA = 12
| 12mA drive current More...
const byte | FT_DRIVE_CURRENT_16MA = 16
| 16mA drive current More...

## Detailed Description

Valid values for drive current options on FT2232H, FT4232H and FT232H devices.

## Member Data Documentation

## ◆ FT_DRIVE_CURRENT_12MA

const byte FTD2XX_NET.FTDI.FT_DRIVE_CURRENT.FT_DRIVE_CURRENT_12MA = 12

12mA drive current

## ◆ FT_DRIVE_CURRENT_16MA

const byte FTD2XX_NET.FTDI.FT_DRIVE_CURRENT.FT_DRIVE_CURRENT_16MA = 16

16mA drive current

## ◆ FT_DRIVE_CURRENT_4MA

const byte FTD2XX_NET.FTDI.FT_DRIVE_CURRENT.FT_DRIVE_CURRENT_4MA = 4

4mA drive current

## ◆ FT_DRIVE_CURRENT_8MA

const byte FTD2XX_NET.FTDI.FT_DRIVE_CURRENT.FT_DRIVE_CURRENT_8MA = 8

8mA drive current

The documentation for this class was generated from the following file:

- C:/PROJECTS/C#/BSL430.NET/src/BSL430.NET/FTD2XX_NET.cs