BSL430.NET 1.2.1

Public Attributes | List of all members
FTD2XX_NET.FTDI.FT_EVENTS Class Reference

FTDI device event types that can be monitored More...

## Public Attributes
const UInt32 | FT_EVENT_RXCHAR = 0x00000001
| Event on receive character More...
const UInt32 | FT_EVENT_MODEM_STATUS = 0x00000002
| Event on modem status change More...
const UInt32 | FT_EVENT_LINE_STATUS = 0x00000004
| Event on line status change More...

## Detailed Description

FTDI device event types that can be monitored

## Member Data Documentation

## ◆ FT_EVENT_LINE_STATUS

const UInt32 FTD2XX_NET.FTDI.FT_EVENTS.FT_EVENT_LINE_STATUS = 0x00000004

Event on line status change

## ◆ FT_EVENT_MODEM_STATUS

const UInt32 FTD2XX_NET.FTDI.FT_EVENTS.FT_EVENT_MODEM_STATUS = 0x00000002

Event on modem status change

## ◆ FT_EVENT_RXCHAR

const UInt32 FTD2XX_NET.FTDI.FT_EVENTS.FT_EVENT_RXCHAR = 0x00000001

Event on receive character

The documentation for this class was generated from the following file:

- C:/PROJECTS/C#/BSL430.NET/src/BSL430.NET/FTD2XX_NET.cs