BSL430.NET 1.2.1

Public Attributes | List of all members
FTD2XX_NET.FTDI.FT_MODEM_STATUS Class Reference

Modem status bit definitions More...

## Public Attributes
const byte | FT_CTS = 0x10
| Clear To Send (CTS) modem status More...
const byte | FT_DSR = 0x20
| Data Set Ready (DSR) modem status More...
const byte | FT_RI = 0x40
| Ring Indicator (RI) modem status More...
const byte | FT_DCD = 0x80
| Data Carrier Detect (DCD) modem status More...

## Detailed Description

Modem status bit definitions

## Member Data Documentation

## ◆ FT_CTS

const byte FTD2XX_NET.FTDI.FT_MODEM_STATUS.FT_CTS = 0x10

Clear To Send (CTS) modem status

## ◆ FT_DCD

const byte FTD2XX_NET.FTDI.FT_MODEM_STATUS.FT_DCD = 0x80

Data Carrier Detect (DCD) modem status

## ◆ FT_DSR

const byte FTD2XX_NET.FTDI.FT_MODEM_STATUS.FT_DSR = 0x20

Data Set Ready (DSR) modem status

## ◆ FT_RI

const byte FTD2XX_NET.FTDI.FT_MODEM_STATUS.FT_RI = 0x40

Ring Indicator (RI) modem status

The documentation for this class was generated from the following file:

- C:/PROJECTS/C#/BSL430.NET/src/BSL430.NET/FTD2XX_NET.cs