BSL430.NET 1.2.1

FTD2XX_NET.FTDI Member List

This is the complete list of members for FTD2XX_NET.FTDI, including all inherited members.

Close() | FTD2XX_NET.FTDI |
CyclePort() | FTD2XX_NET.FTDI |
EEReadUserArea(byte[] UserAreaDataBuffer, ref UInt32 numBytesRead) | FTD2XX_NET.FTDI |
EEUserAreaSize(ref UInt32 UASize) | FTD2XX_NET.FTDI |
EEWriteUserArea(byte[] UserAreaDataBuffer) | FTD2XX_NET.FTDI |
EraseEEPROM() | FTD2XX_NET.FTDI |
FT_DEVICE enum name | FTD2XX_NET.FTDI |
FT_STATUS enum name | FTD2XX_NET.FTDI |
FTDI() | FTD2XX_NET.FTDI |
FTDI(String path) | FTD2XX_NET.FTDI |
GetCOMPort(out string ComPortName) | FTD2XX_NET.FTDI |
GetDescription(out string Description) | FTD2XX_NET.FTDI |
GetDeviceID(ref UInt32 DeviceID) | FTD2XX_NET.FTDI |
GetDeviceList(FT_DEVICE_INFO_NODE[] devicelist) | FTD2XX_NET.FTDI |
GetDeviceType(ref FT_DEVICE DeviceType) | FTD2XX_NET.FTDI |
GetDriverVersion(ref UInt32 DriverVersion) | FTD2XX_NET.FTDI |
GetEventType(ref UInt32 EventType) | FTD2XX_NET.FTDI |
GetLatency(ref byte Latency) | FTD2XX_NET.FTDI |
GetLibraryVersion(ref UInt32 LibraryVersion) | FTD2XX_NET.FTDI |
GetLineStatus(ref byte LineStatus) | FTD2XX_NET.FTDI |
GetModemStatus(ref byte ModemStatus) | FTD2XX_NET.FTDI |
GetNumberOfDevices(ref UInt32 devcount) | FTD2XX_NET.FTDI |
GetPinStates(ref byte BitMode) | FTD2XX_NET.FTDI |
GetRxBytesAvailable(ref UInt32 RxQueue) | FTD2XX_NET.FTDI |
GetSerialNumber(out string SerialNumber) | FTD2XX_NET.FTDI |
GetTxBytesWaiting(ref UInt32 TxQueue) | FTD2XX_NET.FTDI |
InTransferSize(UInt32 InTransferSize) | FTD2XX_NET.FTDI |
IsOpen | FTD2XX_NET.FTDI |
OpenByDescription(string description) | FTD2XX_NET.FTDI |
OpenByIndex(UInt32 index) | FTD2XX_NET.FTDI |
OpenByLocation(UInt32 location) | FTD2XX_NET.FTDI |
OpenBySerialNumber(string serialnumber) | FTD2XX_NET.FTDI |
Purge(UInt32 purgemask) | FTD2XX_NET.FTDI |
Read(byte[] dataBuffer, UInt32 numBytesToRead, ref UInt32 numBytesRead) | FTD2XX_NET.FTDI |
Read(out string dataBuffer, UInt32 numBytesToRead, ref UInt32 numBytesRead) | FTD2XX_NET.FTDI |
ReadEEPROMLocation(UInt32 Address, ref UInt16 EEValue) | FTD2XX_NET.FTDI |
ReadFT2232EEPROM(FT2232_EEPROM_STRUCTURE ee2232) | FTD2XX_NET.FTDI |
ReadFT2232HEEPROM(FT2232H_EEPROM_STRUCTURE ee2232h) | FTD2XX_NET.FTDI |
ReadFT232BEEPROM(FT232B_EEPROM_STRUCTURE ee232b) | FTD2XX_NET.FTDI |
ReadFT232HEEPROM(FT232H_EEPROM_STRUCTURE ee232h) | FTD2XX_NET.FTDI |
ReadFT232REEPROM(FT232R_EEPROM_STRUCTURE ee232r) | FTD2XX_NET.FTDI |
ReadFT4232HEEPROM(FT4232H_EEPROM_STRUCTURE ee4232h) | FTD2XX_NET.FTDI |
ReadXSeriesEEPROM(FT_XSERIES_EEPROM_STRUCTURE eeX) | FTD2XX_NET.FTDI |
Reload(UInt16 VendorID, UInt16 ProductID) | FTD2XX_NET.FTDI |
Rescan() | FTD2XX_NET.FTDI |
ResetDevice() | FTD2XX_NET.FTDI |
ResetPort() | FTD2XX_NET.FTDI |
RestartInTask() | FTD2XX_NET.FTDI |
SetBaudRate(UInt32 BaudRate) | FTD2XX_NET.FTDI |
SetBitMode(byte Mask, byte BitMode) | FTD2XX_NET.FTDI |
SetBreak(bool Enable) | FTD2XX_NET.FTDI |
SetCharacters(byte EventChar, bool EventCharEnable, byte ErrorChar, bool ErrorCharEnable) | FTD2XX_NET.FTDI |
SetDataCharacteristics(byte DataBits, byte StopBits, byte Parity) | FTD2XX_NET.FTDI |
SetDeadmanTimeout(UInt32 DeadmanTimeout) | FTD2XX_NET.FTDI |
SetDTR(bool Enable) | FTD2XX_NET.FTDI |
SetEventNotification(UInt32 eventmask, EventWaitHandle eventhandle) | FTD2XX_NET.FTDI |
SetFlowControl(UInt16 FlowControl, byte Xon, byte Xoff) | FTD2XX_NET.FTDI |
SetLatency(byte Latency) | FTD2XX_NET.FTDI |
SetResetPipeRetryCount(UInt32 ResetPipeRetryCount) | FTD2XX_NET.FTDI |
SetRTS(bool Enable) | FTD2XX_NET.FTDI |
SetTimeouts(UInt32 ReadTimeout, UInt32 WriteTimeout) | FTD2XX_NET.FTDI |
StopInTask() | FTD2XX_NET.FTDI |
VendorCmdGet(UInt16 request, byte[] buf, UInt16 len) | FTD2XX_NET.FTDI |
VendorCmdSet(UInt16 request, byte[] buf, UInt16 len) | FTD2XX_NET.FTDI |
Write(byte[] dataBuffer, Int32 numBytesToWrite, ref UInt32 numBytesWritten) | FTD2XX_NET.FTDI |
Write(byte[] dataBuffer, UInt32 numBytesToWrite, ref UInt32 numBytesWritten) | FTD2XX_NET.FTDI |
Write(string dataBuffer, Int32 numBytesToWrite, ref UInt32 numBytesWritten) | FTD2XX_NET.FTDI |
Write(string dataBuffer, UInt32 numBytesToWrite, ref UInt32 numBytesWritten) | FTD2XX_NET.FTDI |
WriteEEPROMLocation(UInt32 Address, UInt16 EEValue) | FTD2XX_NET.FTDI |
WriteFT2232EEPROM(FT2232_EEPROM_STRUCTURE ee2232) | FTD2XX_NET.FTDI |
WriteFT2232HEEPROM(FT2232H_EEPROM_STRUCTURE ee2232h) | FTD2XX_NET.FTDI |
WriteFT232BEEPROM(FT232B_EEPROM_STRUCTURE ee232b) | FTD2XX_NET.FTDI |
WriteFT232HEEPROM(FT232H_EEPROM_STRUCTURE ee232h) | FTD2XX_NET.FTDI |
WriteFT232REEPROM(FT232R_EEPROM_STRUCTURE ee232r) | FTD2XX_NET.FTDI |
WriteFT4232HEEPROM(FT4232H_EEPROM_STRUCTURE ee4232h) | FTD2XX_NET.FTDI |
WriteXSeriesEEPROM(FT_XSERIES_EEPROM_STRUCTURE eeX) | FTD2XX_NET.FTDI |