BSL430.NET 1.2.1

Public Attributes | List of all members
FTD2XX_NET.FTDI.FT_EEPROM_DATA Class Reference

Common EEPROM elements for all devices. Inherited to specific device type EEPROMs. More...

Inheritance diagram for FTD2XX_NET.FTDI.FT_EEPROM_DATA:

## Public Attributes
UInt16 | VendorID = 0x0403
| Vendor ID as supplied by the USB Implementers Forum More...
UInt16 | ProductID = 0x6001
| Product ID More...
string | Manufacturer = "FTDI"
| Manufacturer name string More...
string | ManufacturerID = "FT"
| Manufacturer name abbreviation to be used as a prefix for automatically generated serial numbers More...
string | Description = "USB-Serial Converter"
| Device description string More...
string | SerialNumber = ""
| Device serial number string More...
UInt16 | MaxPower = 0x0090
| Maximum power the device needs More...
bool | SelfPowered = false
| Indicates if the device has its own power supply (self-powered) or gets power from the USB port (bus-powered) More...
bool | RemoteWakeup = false
| Determines if the device can wake the host PC from suspend by toggling the RI line More...

## Detailed Description

Common EEPROM elements for all devices. Inherited to specific device type EEPROMs.

## Member Data Documentation

## ◆ Description

string FTD2XX_NET.FTDI.FT_EEPROM_DATA.Description = "USB-Serial Converter"

Device description string

## ◆ Manufacturer

string FTD2XX_NET.FTDI.FT_EEPROM_DATA.Manufacturer = "FTDI"

Manufacturer name string

## ◆ ManufacturerID

string FTD2XX_NET.FTDI.FT_EEPROM_DATA.ManufacturerID = "FT"

Manufacturer name abbreviation to be used as a prefix for automatically generated serial numbers

## ◆ MaxPower

UInt16 FTD2XX_NET.FTDI.FT_EEPROM_DATA.MaxPower = 0x0090

Maximum power the device needs

## ◆ ProductID

UInt16 FTD2XX_NET.FTDI.FT_EEPROM_DATA.ProductID = 0x6001

Product ID

## ◆ RemoteWakeup

bool FTD2XX_NET.FTDI.FT_EEPROM_DATA.RemoteWakeup = false

Determines if the device can wake the host PC from suspend by toggling the RI line

## ◆ SelfPowered

bool FTD2XX_NET.FTDI.FT_EEPROM_DATA.SelfPowered = false

Indicates if the device has its own power supply (self-powered) or gets power from the USB port (bus-powered)

## ◆ SerialNumber

string FTD2XX_NET.FTDI.FT_EEPROM_DATA.SerialNumber = ""

Device serial number string

## ◆ VendorID

UInt16 FTD2XX_NET.FTDI.FT_EEPROM_DATA.VendorID = 0x0403

Vendor ID as supplied by the USB Implementers Forum

The documentation for this class was generated from the following file:

- C:/PROJECTS/C#/BSL430.NET/src/BSL430.NET/FTD2XX_NET.cs