#N canvas 459 23 560 556 10;
#X obj 5 529 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 3 375 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 5 458 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 5 501 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 58 389 cnv 17 3 40 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 101 468 cnv 17 3 26 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 85 388 signal;
#X text 144 388 - input signal to detect transitions;
#X obj 58 435 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 90 435 float;
#X text 133 467 float;
#X text 188 509 (none);
#X floatatom 299 201 0 0 0 0 - - - 0;
#X obj 218 227 cyclone/spike~;
#X text 274 254 ms;
#X text 143 435 - set refractory period \, the maximal reporting rate, f 58;
#X text 329 200 set refractory frequency;
#X obj 218 165 cyclone/train~ 500;
#X obj 218 283 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 238 196 bng 19 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X text 97 405 bang;
#X text 73 92 [spike~] reports intervals of zero to non-zero transitions from the signal input. The refractory period is set at the second inlet \, which defines how soon after detecting a transition the spike~ object will report the next instance.;
#X obj 218 255 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 143 405 -;
#X text 155 405 restarts the countdown of the refractory period from the time at which the bang was received;
#X text 186 467 -;
#X text 198 467 interval in ms since last 0 to non-0 transition (including the refractory period \, if one is set);
#X obj 500 69 cyclone/dsponoff~;
#X obj 4 3 ./header spike~;
#X text 25 59 Report zero to non-zero transition intervals;
#X obj 44 314 timer;
#X obj 44 337 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 44 265 threshold~ 1 0 0.1 0;
#X obj 44 287 t b b;
#X text 108 325 This is a Vanilla alternative, f 17;
#X obj 464 349 open-else;
#X text 467 281 click;
#X text 242 311 Plugdata users or those with ELSE can also use [else/status~] with as [else/detect~] an alternative., f 33;
#X msg 464 301 status~;
#X msg 475 324 detect~;
#X connect 12 0 13 1;
#X connect 13 0 22 0;
#X connect 17 0 13 0;
#X connect 17 0 32 0;
#X connect 19 0 13 0;
#X connect 22 0 18 0;
#X connect 30 0 31 0;
#X connect 32 0 33 0;
#X connect 33 0 30 0;
#X connect 33 1 30 1;
#X connect 38 0 35 0;
#X connect 39 0 35 0;
