#N canvas 338 91 566 581 10;
#X obj 3 376 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 3 454 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 3 518 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 102 385 cnv 17 3 35 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 102 429 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 102 488 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 102 465 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 3 573 cnv 3 550 3 empty empty empty 0 0 0 4 #fcfcfc #000000 0;
#X obj 3 553 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X text 130 528 (none);
#X text 136 403 float;
#X text 136 431 float;
#X text 136 466 float;
#X text 136 489 float;
#X text 117 152 Amplitude;
#X text 323 153 Phase;
#X obj 182 269 nbx 8 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 275 268 nbx 8 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 147 267 Real;
#X text 360 268 Imaginary;
#X obj 182 152 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 263 152 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 142 386 bang;
#X text 190 386 - converts the last received coordinates pair;
#X obj 206 194 t bang float;
#X obj 182 226 cyclone/poltocar;
#X text 86 88 [poltocar] converts polar coordinates (amplitude / phase) to cartesian coordinates (real / imaginary).;
#X text 190 403 - amplitude from the polar coordinates, f 43;
#X text 191 431 - phase (in radians) from the polar coordinates;
#X text 191 466 - real part of the cartesian form;
#X text 191 489 - imaginary part of the cartesian form, f 51;
#X obj 2 3 ./header poltocar;
#X text 23 61 Polar to cartesian conversion;
#X text 19 328 see also:;
#X obj 445 342 open-else;
#X text 448 298 click:;
#X obj 87 319 cyclone/poltocar~;
#X obj 87 339 cyclone/cartopol;
#X msg 445 321 pol2car;
#X text 215 319 Plugdata users or those with ELSE can also use [else/pol2car] as an alternative, f 33;
#X connect 20 0 25 0;
#X connect 21 0 24 0;
#X connect 24 0 25 0;
#X connect 24 1 25 1;
#X connect 25 0 16 0;
#X connect 25 1 17 0;
#X connect 38 0 34 0;
