#N canvas 359 23 564 658 10;
#X declare -stdpath ./;
#X obj 5 629 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 8 510 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 9 561 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 9 598 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 102 518 cnv 17 3 37 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 102 571 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 166 518 bang;
#X text 153 571 signal;
#X obj 145 328 print~;
#X obj 215 337 cyclone/allpass~ 40 40 0.5;
#X text 265 210 set impulse value(s);
#X text 130 537 set <list>;
#X text 204 518 - generates impulse;
#X text 204 571 - generated impulse;
#X text 227 318 test your reverberator:;
#X obj 145 261 bng 19 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X msg 145 200 set -1 0.25 1 0.5;
#X msg 215 224 set 1;
#X text 204 606 - amplitude value(s) of the impulse (default 1);
#X text 204 537 - sets impulse amplitude value(s) \, maximum of 256 values;
#X obj 500 69 cyclone/dsponoff~;
#X obj 215 373 output~;
#X text 146 607 1) list;
#X obj 2 3 ./header click~;
#X text 25 58 Impulse generator;
#X obj 55 376 declare -stdpath ./;
#X obj 215 290 cyclone/click~;
#X text 153 459 Plugdata users or those with ELSE can also use [else/impseq~], f 34;
#X text 57 93 [click~] generates an impulse when receiving a bang. An impulse is a single sample with a value of one followed by zeros \, and this is the default impulse generated by [click~] \, but you can can also set an impulse with a different amplitude value or even as a list of values (for band limited impulses - maximum is 256 sample values)., f 63;
#X text 81 465 see also:;
#X obj 397 476 open-else;
#X msg 397 449 impseq~;
#X text 455 449 <-- click;
#X connect 9 0 21 0;
#X connect 15 0 8 0;
#X connect 15 0 26 0;
#X connect 16 0 15 0;
#X connect 16 0 26 0;
#X connect 17 0 15 0;
#X connect 17 0 26 0;
#X connect 26 0 8 0;
#X connect 26 0 9 0;
#X connect 31 0 30 0;
