#N canvas 473 42 565 613 10;
#X obj 4 577 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 4 438 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 4 497 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 4 537 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 84 507 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 117 446 signal;
#X text 208 547 (none);
#X text 117 508 signal;
#X obj 84 448 cnv 17 3 42 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 228 244 cyclone/change~;
#X obj 228 211 line~;
#X text 179 149 increasing;
#X text 259 148 decreasing;
#X obj 228 308 tgl 20 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000 0 1;
#X text 255 311 Signal is changing;
#X floatatom 284 212 5 0 0 0 - - - 0;
#X text 123 465 float;
#X text 62 93 Use [change~] to detect if signal is changing and its direction. It outputs "1" if the signal is increasing \, "-1" if it's decreasing and "0" if it doesn't change.;
#X text 178 446 - signal to detect change & direction;
#X text 178 465 - when DSP is off \, sets an internal value to be compared with incoming signal when DSP is on.;
#X text 177 508 - 1 when increasing \, -1 when decreasing and 0 for no change;
#X obj 228 278 cyclone/snapshot~ 1;
#X text 320 212 internal value;
#X obj 495 69 cyclone/dsponoff~;
#X obj 4 3 ./header change~;
#X text 17 61 Detect signal change & direction;
#X floatatom 228 333 5 0 0 0 - - - 0;
#X obj 92 283 cyclone/snapshot~ 1;
#X floatatom 92 310 13 0 0 0 - - - 0;
#X msg 178 171 -1 \, 1 2500;
#X msg 260 170 1 \, -1 2500;
#X text 57 385 see also:;
#X text 135 379 Plugdata users or those with ELSE can also use [else/changed2~] and [else/changed~], f 42;
#X obj 417 402 open-else;
#X text 489 375 click:;
#X msg 417 351 changed2~;
#X msg 427 375 changed~;
#X connect 9 0 21 0;
#X connect 10 0 9 0;
#X connect 10 0 27 0;
#X connect 13 0 26 0;
#X connect 15 0 9 0;
#X connect 21 0 13 0;
#X connect 27 0 28 0;
#X connect 29 0 10 0;
#X connect 30 0 10 0;
#X connect 35 0 33 0;
#X connect 36 0 33 0;
