#N canvas 306 50 563 684 10;
#X obj 8 576 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 8 617 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 86 588 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 86 477 cnv 17 3 60 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 8 467 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 86 477 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 134 478 signal;
#X text 146 506 bang;
#X msg 254 255 set 10;
#X text 135 587 signal;
#X text 120 627 1) float;
#X obj 70 290 cyclone/plusequals~;
#X text 187 506 - resets initial stored value to 0;
#X text 188 476 - signal value is accumulated. Accumulated value is output only if a signal is connected;
#X obj 83 254 bng 19 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 5 652 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 85 543 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 134 543 signal;
#X text 105 523 set <float>;
#X text 187 523 - sets the stored value to that number;
#X text 186 543 - signal different than 0 resets initial stored value to 0;
#X text 190 587 - each sample is the sum of all previous input samples;
#X text 186 627 - sets the initial stored value for the sum (default 0);
#X obj 70 220 sig~ 0.0001;
#X text 72 92 [plusequals~] or [+=~] accumulates the received values. Each input sample is added to the previous ones for a running sum. So \, started at 0 \, a signal consisting of 1 values outputs the sequence (1 \, 2 \, 3 \, 4 \, etc...).;
#X text 106 255 <= reset =>;
#X text 73 154 The internal sum can be reset to 0 with a bang (left inlet) or a signal different than 0 in the right inlet (with sample accuracy) - or also set to any value (with the set message).;
#X obj 181 225 cyclone/train~ 2000 0;
#X text 321 224 <= impulse (value of 1;
#X text 362 240 every 2 seconds);
#X obj 499 69 cyclone/dsponoff~;
#X obj 455 345 cyclone-help;
#X text 450 324 Please check:;
#X obj 254 291 cyclone/+=~;
#X obj 3 5 ./header +=~;
#X text 22 61 Signal accumulator;
#X obj 70 331 cyclone/snapshot~ 1;
#X floatatom 70 363 5 0 0 0 - - - 12;
#X obj 254 326 cyclone/snapshot~ 1;
#X floatatom 254 358 5 0 0 0 - - - 12;
#X obj 426 433 open-else;
#X text 464 407 click;
#X text 83 418 see also:;
#X msg 426 407 add~;
#X text 152 411 Plugdata users or those with ELSE can also use [else/add~] as an alternative, f 42;
#X connect 8 0 33 0;
#X connect 11 0 36 0;
#X connect 14 0 11 0;
#X connect 23 0 11 0;
#X connect 27 0 11 1;
#X connect 27 0 33 0;
#X connect 33 0 38 0;
#X connect 36 0 37 0;
#X connect 38 0 39 0;
#X connect 43 0 40 0;
