#N canvas 468 23 561 529 10;
#X obj 2 377 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 433 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 469 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 91 386 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 91 444 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 91 408 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 120 159 tgl 20 0 empty empty empty 17 7 0 10 #d0d0d0 #000000 #000000 0 1;
#X obj 2 503 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X text 173 408 -;
#X text 133 408 float;
#X text 173 386 -;
#X text 115 386 anything;
#X text 173 444 -;
#X text 115 444 anything;
#X text 173 476 -;
#X text 115 476 1) float;
#X obj 120 217 random 100;
#X obj 120 193 metro 50;
#X floatatom 120 247 5 0 0 0 - - - 0;
#X obj 198 273 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 198 207 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X floatatom 321 221 5 0 0 0 - - - 0;
#X text 318 201 change time limit;
#X text 188 386 any message input message to be speed limited;
#X text 188 408 changes the time limit (in ms), f 32;
#X text 359 221 milliseconds;
#X text 79 86 [speedlim] only allows messages through if a given time has elapsed since the previous input/output. Otherwise \, it waits until that time passes and then sends the last received message since the previous output (ignoring the others).;
#X text 188 444 the last input in the time interval after last output, f 54;
#N canvas 716 105 393 604 more 0;
#X obj 154 274 float;
#X obj 208 199 loadbang;
#X obj 208 221 tgl 15 0 empty empty empty 17 7 0 10 #fcfcfc #000000 #000000 0 1;
#X obj 154 302 change;
#X floatatom 150 215 5 0 0 0 - - - 0;
#X floatatom 154 335 5 0 0 0 - - - 0;
#X obj 208 242 metro 1000;
#X text 24 159 The [speedlimit] object is similar to this construction:;
#X msg 104 449 1 2 3;
#X obj 161 542 print;
#X msg 161 449 x;
#X msg 196 449 a b c;
#X msg 194 474 symbol dog;
#X msg 142 421 list one 2 3;
#X obj 153 66 ctlin 1 1;
#X text 138 34 filter MIDI input;
#X text 74 391 it works with any kind of message;
#X obj 153 105 cyclone/speedlim 100;
#X obj 161 507 cyclone/speedlim 1500;
#X connect 0 0 3 0;
#X connect 1 0 2 0;
#X connect 2 0 6 0;
#X connect 3 0 5 0;
#X connect 4 0 0 1;
#X connect 6 0 0 0;
#X connect 8 0 18 0;
#X connect 10 0 18 0;
#X connect 11 0 18 0;
#X connect 12 0 18 0;
#X connect 13 0 18 0;
#X connect 14 0 17 0;
#X connect 18 0 9 0;
#X restore 474 269 pd more;
#X obj 198 244 cyclone/speedlim 1000;
#X text 187 476 initial time limit (default 0 - no limit);
#X obj 5 5 ./header speedlim;
#X text 22 63 Limit the speed of messages;
#X text 77 324 see also:;
#X obj 421 335 open-else;
#X text 461 306 click;
#X msg 421 307 limit;
#X text 149 317 Plugdata users or those with ELSE can also use [else/limit] as an alternative., f 40;
#X connect 6 0 17 0;
#X connect 16 0 18 0;
#X connect 16 0 29 0;
#X connect 17 0 16 0;
#X connect 20 0 29 0;
#X connect 21 0 29 1;
#X connect 29 0 19 0;
#X connect 36 0 34 0;
