#N canvas 453 79 561 534 10;
#X obj 3 341 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 3 417 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 3 455 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 84 350 cnv 17 3 60 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 84 426 cnv 17 3 17 empty empty n 5 9 0 16 #dcdcdc #9c9c9c 0;
#X msg 223 168 1;
#X msg 254 168 2;
#X msg 285 168 3;
#X msg 204 143 1 2 3;
#X obj 204 249 bng 19 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X msg 153 164 set 1;
#X text 136 349 anything;
#X text 160 462 -;
#X text 102 462 1) float;
#X text 160 480 -;
#X text 102 480 2) float;
#X obj 3 503 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X text 118 377 set <float>;
#X text 195 395 - switches output mode, f 51;
#X text 100 395 thresh <float>;
#X obj 204 229 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 247 228 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 291 228 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 77 86 Each incoming number is sent to the next outlet \, wrapping around to the first outlet after the last has been reached \, completing a cycle in a "round-robin scheduling" way.;
#X text 195 378 - sets the next output outlet (starting at 0), f 51;
#X text 195 349 - any message type. Messages with more than one element outputs each element to a different outlet;
#X obj 204 204 cyclone/cycle 3;
#X text 174 480 mode: Non-0 sets to "event sensitive mode" (default 0);
#N canvas 749 171 456 477 mode 0;
#X msg 169 270 1;
#X msg 200 270 2;
#X msg 230 270 3;
#X msg 156 240 thresh \$1;
#X obj 156 357 cyclone/cycle 3 1;
#X msg 233 322 1 \, 2 \, 3;
#X obj 156 215 tgl 15 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000 0 1;
#X obj 156 409 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 156 384 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 205 408 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 205 383 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 255 407 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 255 383 nbx 2 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X msg 95 322 set 1;
#X msg 233 297 1 2;
#X text 54 108 Examples of separate events include messages with delays between them \, and messages triggered by successive mouse clicks or MIDI events.;
#X text 55 155 A stream of items separated by commas in a message box is considered a single event.;
#X text 53 34 In the event sensitive mode (set with the second argument or with the "tresh" message) \, any new event will restart the output from the leftmost outlet. In the default mode (0) \, the values cycle through all the outlets \, regardless of whether they are attached to separate events or not.;
#X text 177 213 changes the mode (1 event sensitive);
#X connect 0 0 4 0;
#X connect 1 0 4 0;
#X connect 2 0 4 0;
#X connect 3 0 4 0;
#X connect 4 0 8 0;
#X connect 4 1 10 0;
#X connect 4 2 12 0;
#X connect 5 0 4 0;
#X connect 6 0 3 0;
#X connect 8 0 7 0;
#X connect 10 0 9 0;
#X connect 12 0 11 0;
#X connect 13 0 4 0;
#X connect 14 0 4 0;
#X restore 426 231 pd mode example;
#X text 112 428 float/symbol;
#X text 194 428 - a float or a symbol atom element \, depending on the input;
#X text 174 462 sets number of outlets (default 1 \, max 128), f 60;
#X obj 2 4 ./header cycle;
#X text 23 60 Round-robin messages to outlets;
#X obj 247 248 bng 19 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 291 247 bng 19 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X text 112 301 see also:;
#X obj 185 302 cyclone/bucket;
#X obj 286 302 cyclone/spray, f 14;
#X connect 5 0 26 0;
#X connect 6 0 26 0;
#X connect 7 0 26 0;
#X connect 8 0 26 0;
#X connect 10 0 26 0;
#X connect 20 0 9 0;
#X connect 21 0 34 0;
#X connect 22 0 35 0;
#X connect 26 0 20 0;
#X connect 26 1 21 0;
#X connect 26 2 22 0;
