#N canvas 368 23 565 688 10;
#X declare -stdpath ./;
#X obj 6 656 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 6 538 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 6 593 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 6 625 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 128 547 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 128 602 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 194 547 signal;
#X text 193 602 signal;
#X text 180 633 1) float;
#X obj 128 568 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X floatatom 217 204 7 -10 10 0 - - - 0;
#X obj 220 183 hsl 128 15 -10 10 0 1 empty empty empty 45 9 1 12 #dcdcdc #000000 #000000 6300 1;
#X obj 89 204 osc~ 206;
#X text 248 568 - drive factor;
#X text 248 633 - initial drive factor;
#X text 245 183 drive factor;
#X text 158 568 float/signal;
#X text 248 602 - the distorted signal;
#X obj 217 252 line~;
#X msg 217 227 \$1 20;
#X obj 89 241 cyclone/overdrive~;
#X text 248 546 - the signal to be distorted;
#X obj 502 72 cyclone/dsponoff~;
#X obj 89 372 output~;
#X obj 2 2 ./header overdrive~;
#X text 22 61 Analog overdrive simulation;
#X obj 359 239 declare -stdpath ./;
#X obj 270 296 cnv 19 250 110 empty empty empty 20 12 0 12 #e0e0e0 #404040 0;
#N canvas 0 50 450 250 (subpatch) 0;
#X array \$0-overdrive 441 float 0;
#X coords 0 1 440 -1 252 112 1 0 0;
#X restore 269 295 graph;
#X obj 118 288 metro 250;
#X obj 105 312 tabwrite~ \$0-overdrive;
#X obj 118 267 loadbang;
#X obj 89 342 clip~ -1 1;
#X text 27 91 [overdrive~] simulates the "soft clipping" of and overdriven tube-based circuit by applying a non-linear transfer function to the incoming signal. If the "drive factor" is 1 \, the signal is unchanged. Increasing the "drive" increases the amount of distortion. If the "drive" is less than 1 \, then it causes a different kind of distortion. If the "drive" is less than 0 \, VERY LOUD distortion can result \, so be careful (here we use [clip~])!, f 71;
#X obj 408 496 open-else;
#X text 455 470 click;
#X text 75 481 see also:;
#X msg 408 470 drive~;
#X text 144 474 Plugdata users or those with ELSE can also use [else/drive~] as an alternative, f 40;
#X connect 10 0 19 0;
#X connect 11 0 10 0;
#X connect 12 0 20 0;
#X connect 18 0 20 1;
#X connect 19 0 18 0;
#X connect 20 0 32 0;
#X connect 20 0 30 0;
#X connect 29 0 30 0;
#X connect 31 0 29 0;
#X connect 32 0 23 0;
#X connect 37 0 34 0;
