#N canvas 329 63 564 604 10;
#X obj 1 459 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 1 507 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 1 544 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 84 516 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 84 473 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 158 516 signal;
#X text 157 554 (none);
#X obj 5 576 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 151 215 nbx 5 14 -100 0 1 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 154 184 hsl 180 15 -100 0 0 0 empty empty empty -2 -8 0 10 #dcdcdc #000000 #000000 0 1;
#X text 122 473 signal/float;
#X text 78 92 [atodb~] takes any given signal representing a dBFS amplitude value and outputs a signal which is a linear amplitude conversion of the input.;
#X text 76 141 Conversion expression: amp = pow(10 \, dBFS / 20);
#X obj 151 277 cyclone/dbtoa~;
#X text 210 473 - value representing dBFS amplitude;
#X text 210 518 - corresponding linear amplitude value;
#X text 244 347 Linear Amplitude;
#X obj 151 240 sig~ -100;
#X obj 498 71 cyclone/dsponoff~;
#X obj 5 5 ./header dbtoa~;
#X text 23 61 Convert dBFS to linear amplitude for signals;
#X text 213 214 dBFS;
#X obj 151 316 cyclone/snapshot~ 1;
#X obj 151 346 nbx 9 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 24 405 see also:;
#X text 463 371 click:;
#X obj 465 412 open-else;
#X obj 96 392 cyclone/dbtoa;
#X obj 97 415 cyclone/atodb~;
#X text 202 396 Plugdata users or those with ELSE can also use [else/db2lin~] as an alternative, f 41;
#X msg 465 390 db2lin~;
#X text 361 273 The above is a Vanilla alternative, f 12;
#X obj 372 245 dbtorms~;
#X obj 372 223 +~ 100;
#X connect 8 0 17 0;
#X connect 9 0 8 0;
#X connect 13 0 22 0;
#X connect 17 0 13 0;
#X connect 22 0 23 0;
#X connect 30 0 26 0;
#X connect 33 0 32 0;
