#N canvas 376 87 559 594 10;
#X obj 4 573 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 5 355 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 5 469 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 5 509 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 77 365 cnv 17 3 38 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 121 482 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X floatatom 165 195 5 0 0 0 - - - 0;
#X msg 343 197 2 3 4;
#X text 77 93 [join] takes any type of messages (anything \, float \, symbol \, list) in any inlet and combines them all into an output list.;
#X floatatom 271 197 5 0 0 0 - - - 0;
#X msg 218 144 list x y z;
#X symbolatom 116 172 10 0 0 0 - - - 0;
#X msg 186 143 a;
#X obj 77 409 cnv 17 3 54 empty empty n 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 142 410 anything;
#X text 166 429 bang;
#X text 99 365 triggers <list>;
#N canvas 841 153 425 444 triggers 0;
#X msg 104 199 triggers -1;
#X obj 83 275 cyclone/join 3 @triggers 1 2;
#X msg 83 166 triggers 0 1;
#X msg 52 129 triggers 0 2;
#X text 28 24 You can specify which outlets will trigger (make the inlet "hot") an output with the @triggers attribute. Just include a list of input numbers that match the inlet number. The first (left) inlet is 0 \, the second is 1 and so on (-1 makes all inlets "hot").;
#X text 184 200 all inlets;
#X text 170 166 first and middle inlet;
#X text 137 128 first and right inlet;
#X obj 107 239 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 177 239 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 248 239 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 83 324 unpack float float float;
#X obj 83 369 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 153 369 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X obj 224 369 nbx 5 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X text 264 270 middle and right inlet initially, f 16;
#X connect 0 0 1 0;
#X connect 1 0 11 0;
#X connect 2 0 1 0;
#X connect 3 0 1 0;
#X connect 8 0 1 0;
#X connect 9 0 1 1;
#X connect 10 0 1 2;
#X connect 11 0 12 0;
#X connect 11 1 13 0;
#X connect 11 2 14 0;
#X restore 446 235 pd triggers;
#X text 142 517 1) float;
#X text 203 429 - forces output of stored messages, f 55;
#X text 203 447 - sets a message to that inlet without output, f 55;
#X text 166 481 list;
#X text 200 481 - the list composed of the joined messages;
#X obj 5 542 cnv 3 550 3 empty empty attributes 8 12 0 13 #dcdcdc #000000 0;
#X text 153 550 @triggers <list> - default "0" (left inlet is hot);
#X msg 242 176 symbol hi;
#X msg 324 170 set bim booh bah;
#X obj 306 145 bng 15 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 165 226 cyclone/join 4 @triggers -1;
#X text 106 447 set <anything>;
#X text 202 365 -;
#X text 216 365 define a list of input numbers that trigger an output (make the inlet "hot"): 0 is the first inlet \, 1 the second and so on (-1 makes all inlets "hot"), f 53;
#X text 203 410 - any message type to be combined into a list, f 55;
#X text 201 517 - number of inlets (default 2 \, min 2 / max 255);
#X obj 3 6 ./header join;
#X text 22 61 Combine items into a list;
#X text 47 291 see also:;
#X obj 416 320 open-else;
#X text 459 298 click;
#X msg 416 298 merge;
#X text 150 302 Plugdata users or those with ELSE can also use [else/merge] as an alternative, f 41;
#X listbox 165 255 34 0 0 0 - - - 0;
#X obj 48 311 cyclone/unjoin;
#X obj 110 291 list;
#X connect 6 0 28 0;
#X connect 7 0 28 3;
#X connect 9 0 28 2;
#X connect 10 0 28 1;
#X connect 11 0 28 0;
#X connect 12 0 28 1;
#X connect 25 0 28 2;
#X connect 26 0 28 3;
#X connect 27 0 28 3;
#X connect 28 0 41 0;
#X connect 39 0 37 0;
