#N canvas 360 45 561 523 10;
#X obj 2 353 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 412 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 2 464 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 81 362 cnv 17 3 43 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 81 421 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 242 179 bng 18 250 50 0 empty empty empty 0 -6 0 8 #d0d0d0 #404040 #000000;
#X text 157 471 (none);
#X obj 81 442 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 189 248 bng 18 250 50 0 empty empty empty 17 7 0 10 #d0d0d0 #404040 #000000;
#X obj 276 248 bng 18 250 50 0 empty empty empty 17 7 0 10 #d0d0d0 #404040 #000000;
#X obj 2 516 cnv 1 550 1 empty empty empty 0 0 0 4 #fcfcfc #fcfcfc 0;
#X obj 2 495 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 189 212 cyclone/togedge;
#X text 158 380 -;
#X text 125 380 bang;
#X text 158 361 -;
#X text 119 361 float;
#X text 158 423 -;
#X text 125 423 bang;
#X text 158 442 -;
#X text 125 442 bang;
#X obj 189 180 nbx 3 14 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 10 #dcdcdc #000000 #000000 0 256;
#X msg 221 155 1;
#X msg 189 152 0;
#X msg 158 155 -1;
#X text 73 88 [togedge] sends a bang in the left outlet for "zero to non-zero" transitions \, and a bang in the right outlet for "non-zero to zero" transitions., f 65;
#X text 173 361 number to check for transitions, f 60;
#X text 173 423 if a zero to non-zero transition is detected, f 60;
#X text 173 442 if a non-zero to zero transition is detected, f 60;
#X obj 159 181 tgl 15 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000 0 1;
#X text 173 380 switches the stored value from 0 to non-zero \, or vice versa \, and the change is reported by a corresponding bang output;
#X text 332 168 note that max doesn't deal with floats \, just ints, f 26;
#X obj 2 3 ./header togedge;
#X text 25 61 report zero / non-zero transitions;
#X text 300 249 non-0 to 0;
#X text 117 251 0 to non-0;
#X obj 384 325 open-else;
#X text 435 297 click;
#X text 46 305 see also:;
#X msg 384 297 status;
#X text 117 302 Plugdata users or those with ELSE can also use [else/status] as an alternative., f 42;
#X connect 5 0 12 0;
#X connect 12 0 8 0;
#X connect 12 1 9 0;
#X connect 21 0 12 0;
#X connect 22 0 21 0;
#X connect 23 0 21 0;
#X connect 24 0 21 0;
#X connect 29 0 12 0;
#X connect 39 0 36 0;
