#N canvas 373 38 566 633 10;
#X obj 7 604 cnv 15 552 21 empty empty empty 20 12 0 14 #e0e0e0 #202020 0;
#X obj 7 418 cnv 3 550 3 empty empty inlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 7 502 cnv 3 550 3 empty empty outlets 8 12 0 13 #dcdcdc #000000 0;
#X obj 7 539 cnv 3 550 3 empty empty arguments 8 12 0 13 #dcdcdc #000000 0;
#X obj 120 428 cnv 17 3 37 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X obj 120 475 cnv 17 3 17 empty empty 1 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 152 427 signal;
#X text 207 427 - signal to measure peak amplitude;
#X text 164 446 bang;
#X text 157 512 float;
#X obj 120 512 cnv 17 3 17 empty empty 0 5 9 0 16 #dcdcdc #9c9c9c 0;
#X text 158 475 float;
#X text 113 552 1) float;
#X obj 222 225 *~;
#X obj 282 179 hsl 128 15 0 1 0 0 empty empty empty -2 -8 0 10 #dcdcdc #000000 #000000 0 1;
#X floatatom 279 202 0 0 0 0 - - - 0;
#X obj 222 311 nbx 8 18 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 13 #dcdcdc #000000 #000000 0 256;
#X text 207 446 - reports a peak value;
#X text 207 475 - time interval in ms to report peak values;
#X text 207 512 - reported peak amplitude;
#X obj 222 271 cyclone/peakamp~ 25;
#X obj 89 231 bng 20 250 50 0 empty empty empty 17 7 0 10 #dcdcdc #000000 #000000;
#X obj 89 311 nbx 8 18 -1e+37 1e+37 0 0 empty empty empty 0 -8 0 13 #dcdcdc #000000 #000000 0 256;
#X obj 89 271 cyclone/peakamp~;
#X obj 222 191 noise~;
#X floatatom 356 273 6 0 0 0 - - - 0;
#X obj 359 249 hsl 128 15 0 500 0 0 empty empty empty -2 -8 0 10 #dcdcdc #000000 #000000 0 1;
#X text 397 274 clock time;
#X text 79 213 report;
#X text 91 99 Use the [peakamp~] object to report the absolute value of the peak amplitude of a signal since the last time it was reported. It outputs the peak amplitude when banged or via its own internal clock.;
#X text 185 550 - sets the internal clock \, the interval in milliseconds to output the peak amplitude. If it is 0 (default) \, the clock isn't used and it only outputs when receiving a bang.;
#X obj 499 69 cyclone/dsponoff~;
#X obj 3 4 ./header peakamp~;
#X text 22 61 Signal's peak amplitude;
#X obj 392 379 open-else;
#X text 439 353 click;
#X text 59 364 see also:;
#X msg 392 353 peak~;
#X text 128 357 Plugdata users or those with ELSE can also use [else/peak~] as an alternative, f 40;
#X connect 13 0 20 0;
#X connect 13 0 23 0;
#X connect 14 0 15 0;
#X connect 15 0 13 1;
#X connect 20 0 16 0;
#X connect 21 0 23 0;
#X connect 23 0 22 0;
#X connect 24 0 13 0;
#X connect 25 0 20 1;
#X connect 26 0 25 0;
#X connect 37 0 34 0;
